CLDR Charts | Home | Site Map | Search

# By-Type Chart: Units:Electrical and Frequency

CLDR Version 30 | Index | 2016-10-06

Core Data: | Alphabetic Information | Main Exemplars | Punctuation Exemplars | Index Exemplars | Numbering Systems
Locale Display Names: | Locale Name Patterns | Languages (A-D) | Languages (E-J) | Languages (K-N) | Languages (O-S) | Languages (T-Z) | Scripts | Geographic Regions | Territories (North America) | Territories (South America) | Territories (Africa) | Territories (Europe) | Territories (Asia) | Territories (Oceania) | Locale Variants | Keys
Date & Time: | Fields | Gregorian | Generic | Buddhist | Chinese | Coptic | Dangi | Ethiopic | Ethiopic-Amete-Alem | Hebrew | Indian | Islamic | Japanese | Persian | ROC
Timezones: | Timezone Display Patterns | North America | South America | Africa | Europe | Russia | Western Asia | Central Asia | Eastern Asia | Southern Asia | Southeast Asia | Australasia | Antarctica | Oceania | Unknown Region | Overrides
Numbers: | Symbols | Number Formatting Patterns | Compact Decimal Formatting
Currencies: | North America (C) | South America (C) | Northern/Western Europe | Southern/Eastern Europe | Northern Africa | Western Africa | Middle Africa | Eastern Africa | Southern Africa | Western Asia (C) | Central Asia (C) | Eastern Asia (C) | Southern Asia (C) | Southeast Asia (C) | Oceania (C) | Unknown Region (C)
Units: | Measurement Systems | Duration | Length | Area | Volume | Speed and Acceleration | Mass and Weight | Energy and Power | Electrical and Frequency | Weather | Digital | Coordinates | Other Units | Compound Units
Miscellaneous: | Displaying Lists | Linguistic Elements

ampere
long-displayName | English: ‹amperes›
--- | ---
aimpéir | ·ga·
amp | ·am· ·lo· ·ur· ·zu·
ampe | ·vi·
ampea | ·sw·
ampeerit | ·fi·
amper | ·az· ·hu· ·is· ·sq· ·tk· ·tr· ·uz·
amperai | ·lt·
amperau | ·cy·
ampere | ·af· ·ca· ·da· ·id· ·it· ·ms· ·nb· ·sv·
Ampere | ·de·
ampère | ·gd· ·nl·
Ampère | ·lb·
ampereak | ·eu·
amperes | ·en· ·es_419· ·fil· ·pt·
ampères | ·fr·
amperi | ·bs· ·hr· ·ro· ·sl· ·sr_Latn·
ampēri | ·lv·
amperios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
amperoù | ·br·
amperur | ·fo·
ampery | ·dsb· ·hsb· ·pl·
ampéry | ·cs· ·sk·
amprid | ·et·
ʻamipele | ·to·
αμπέρ | ·el·
ампер | ·kk· ·ky· ·mn· ·sah·
ампери | ·bg· ·mk· ·sr· ·uk·
амперы | ·be· ·ru·
ამპერი | ·ka·
ամպերներ | ·hy·
אמפר | ·he·
آمپر | ·fa· ·mzn·
أمبير | ·ar·
अँपियर | ·mr·
एम्पियर | ·ne·
एम्पीयर | ·hi·
অ্যাম্পিয়ার | ·bn·
ਐਮਪੀਅਰ | ·pa·
એમ્પીયર | ·gu·
ஆம்பியர்கள் | ·ta·
ఆంపియర్స్ | ·te·
ಆಂಪೇರ್‌ಗಳು | ·kn·
ആമ്പിയർ | ·ml·
ඇම්පියර | ·si·
แอมแปร์ | ·th·
အမ်ပီယာ | ·my·
អំពែរ | ·km·
ᏗᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
암페어 | ·ko·
アンペア | ·ja·
安培 | ·yue· ·zh· ·zh_Hant·
long-zero | English: ‹{0} A›
{0} amper | ·cy·
{0} ampēri | ·lv·
{0} أمبير | ·ar·
long-one | English: ‹{0} ampere›
{0} A | ·am· ·ur· ·zu·
{0} aimpéar | ·ga·
{0} ampeeri | ·fi·
{0} amper | ·az· ·br· ·bs· ·cy· ·et· ·hr· ·hu· ·is· ·pl· ·ro· ·sl· ·sq· ·sr_Latn· ·tk· ·tr· ·uz·
{0} ampér | ·cs· ·sk·
{0} ampera | ·fo·
{0} amperas | ·lt·
{0} ampere | ·af· ·ca· ·da· ·dsb· ·en· ·es_419· ·eu· ·fil· ·hsb· ·it· ·nb· ·pt· ·sv·
{0} Ampere | ·de·
{0} ampère | ·gd· ·nl·
{0} Ampère | ·lb·
{0} ampère | ·fr·
{0} amperio | ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
{0} amperiu | ·ast·
{0} ampērs | ·lv·
{0} aмпер | ·kk·
{0} αμπέρ | ·el·
{0} ампер | ·be· ·bg· ·ky· ·mk· ·mn· ·ru· ·sr· ·uk·
{0} ა | ·ka·
{0} ամպեր | ·hy·
{0} آمپر | ·fa·
{0} أمبير | ·ar·
{0} अँपियर | ·mr·
{0} एम्पियर | ·ne·
{0} एम्पीयर | ·hi·
{0} অ্যাম্পিয়ার | ·bn·
{0} ਐਮਪੀਅਰ | ·pa·
{0} એમ્પીયર | ·gu·
{0} ஆம்பியர் | ·ta·
{0} ఆంపియర్ | ·te·
{0} ಆಂಪೇರ್‌ | ·kn·
{0} ആമ്പിയർ | ·ml·
{0} ᎠᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
ampea {0} | ·sw·
אמפר {0} | ·he·
ඇම්පියර {0} | ·si·
long-two | English: ‹{0} A›
{0} aimpéar | ·ga·
{0} amper | ·br· ·cy·
{0} ampera | ·dsb· ·sl·
{0} amperaj | ·hsb·
{0} ampère | ·gd·
{0} אמפר | ·he·
{0} أمبير | ·ar·
long-few | English: ‹{0} A›
{0} aimpéar | ·ga·
{0} amper | ·br· ·cy·
{0} ampera | ·bs· ·hr· ·sr_Latn·
{0} amperai | ·lt·
{0} ampère | ·gd·
{0} amperi | ·ro· ·sl·
{0} ampery | ·dsb· ·hsb· ·pl·
{0} ampéry | ·cs· ·sk·
{0} ампера | ·ru· ·sr·
{0} ампери | ·uk·
{0} амперы | ·be·
{0} أمبير | ·ar·
long-many | English: ‹{0} A›
{0} a amperoù | ·br·
{0} amper | ·cy·
{0} ampéra | ·sk·
{0} ampero | ·lt·
{0} amperów | ·pl·
{0} ampéru | ·cs·
{0} n-aimpéar | ·ga·
{0} ампер | ·be· ·ru·
{0} амперів | ·uk·
{0} אמפר | ·he·
{0} أمبير | ·ar·
long-other | English: ‹{0} amperes›
{0} A | ·am· ·lo· ·ur· ·zu·
{0} aimpéar | ·ga·
{0} ampe | ·vi·
{0} ampeeria | ·fi·
{0} amper | ·az· ·br· ·cy· ·hu· ·is· ·sq· ·tk· ·tr· ·uz·
{0} ampera | ·bs· ·hr· ·pl· ·sr_Latn·
{0} ampere | ·af· ·da· ·eu· ·id· ·it· ·ms· ·nb· ·sv·
{0} Ampere | ·de·
{0} ampère | ·gd· ·nl·
{0} Ampère | ·lb·
{0} amperes | ·ca· ·en· ·es_419· ·pt·
{0} ampères | ·fr·
{0} ampēri | ·lv·
{0} amperios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
{0} amperov | ·sl·
{0} ampérov | ·sk·
{0} amperow | ·dsb· ·hsb·
{0} amperų | ·lt·
{0} ampérů | ·cs·
{0} amperur | ·fo·
{0} amprit | ·et·
{0} aмпер | ·kk·
{0} de amperi | ·ro·
{0} na ampere | ·fil·
{0} αμπέρ | ·el·
{0} ампер | ·ky· ·mn· ·sah·
{0} ампера | ·be· ·bg· ·ru· ·sr· ·uk·
{0} ампери | ·mk·
{0} ა | ·ka·
{0} ամպեր | ·hy·
{0} אמפר | ·he·
{0} آمپر | ·fa· ·mzn·
{0} أمبير | ·ar·
{0} अँपियर | ·mr·
{0} एम्पीयर | ·hi·
{0} অ্যাম্পিয়ার | ·bn·
{0} ਐਮਪੀਅਰ | ·pa·
{0} એમ્પીયર | ·gu·
{0} ஆம்பியர்கள் | ·ta·
{0} ఆంపియర్స్ | ·te·
{0} ಆಂಪೇರ್‌ಗಳು | ·kn·
{0} ആമ്പിയർ | ·ml·
{0} แอมแปร์ | ·th·
{0} အမ်ပီယာ | ·my·
{0} អំពែរ | ·km·
{0} ᏗᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
{0} アンペア | ·ja·
{0} 安培 | ·yue· ·zh_Hant·
{0}एम्पियर | ·ne·
{0}암페어 | ·ko·
{0}安培 | ·zh·
ampea {0} | ·sw·
ʻamipele ʻe {0} | ·to·
ඇම්පියර {0} | ·si·
short-displayName | English: ‹amps›
A | ·bg· ·br· ·ca· ·cs· ·da· ·dsb· ·es· ·eu· ·fi· ·fr· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·nl· ·ro· ·sk· ·sq· ·sr· ·sr_Latn· ·sv· ·tk· ·to· ·vi·
aimpéir | ·ga·
amp | ·all·others·
ampau | ·cy·
ampea | ·sw·
amper | ·tr· ·uz·
ampere | ·af· ·nb·
Ampere | ·de·
amperi | ·bs·
amperur | ·fo·
ampery | ·pl·
amprid | ·et·
amps | ·ast· ·chr· ·en· ·he· ·pt·
αμπέρ | ·el·
А | ·be· ·kk· ·ru· ·uk·
амп | ·ky· ·mn·
амп. | ·mk·
ამპ | ·ka·
Ա | ·hy·
آمپر | ·fa· ·mzn·
أمبير | ·ar·
अँप्स | ·mr·
एम्पी॰ | ·hi·
ਐਮਪੀਅਰ | ·pa·
ஆம்ப். | ·ta·
ఆంప్స్ | ·te·
ಆಂ. | ·kn·
ആമ്പിയർ | ·ml·
ඇම්පිර | ·si·
แอมป์ | ·th·
အမ်ပီယာ | ·my·
អំពែរ | ·km·
アンペア | ·ja·
安培 | ·yue· ·zh· ·zh_Hant·
short-zero | English: ‹{0} A›
{0} A | ·cy· ·lv·
{0} أمبير | ·ar·
short-one | English: ‹{0} A›
{0} A | ·af· ·am· ·ast· ·az· ·be· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hr· ·hsb· ·hu· ·is· ·it· ·kk· ·ky· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tk· ·tr· ·ur· ·uz· ·zu·
{0} А | ·mn· ·ru· ·uk·
{0} ა | ·ka·
{0} Ա | ·hy·
{0} آمپر | ·fa·
{0} أمبير | ·ar·
{0} ए॰ | ·hi·
{0} ஆம். | ·ta·
{0} ఆం | ·te·
{0} ಆಂ. | ·kn·
{0} ആ. | ·ml·
ampea {0} | ·sw·
ඇ {0} | ·si·
short-two | English: ‹{0} A›
{0} A | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} أمبير | ·ar·
short-few | English: ‹{0} A›
{0} A | ·be· ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} А | ·ru· ·uk·
{0} أمبير | ·ar·
short-many | English: ‹{0} A›
{0} A | ·be· ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} А | ·ru· ·uk·
{0} أمبير | ·ar·
short-other | English: ‹{0} A›
{0} A | ·all·others·
{0} А | ·ru· ·sah· ·uk·
{0} ა | ·ka·
{0} Ա | ·hy·
{0} آمپر | ·fa·
{0} أمبير | ·ar·
{0} ए॰ | ·hi·
{0} ஆம். | ·ta·
{0} ఆం | ·te·
{0} ಆಂ. | ·kn·
{0} ആ. | ·ml·
{0} แอมป์ | ·th·
{0} 安培 | ·yue· ·zh_Hant·
{0}A | ·ko·
{0}安 | ·zh·
A ʻe {0} | ·to·
ampea {0} | ·sw·
ඇ {0} | ·si·
narrow-displayName | English: ‹amp›
A | ·cs· ·fi· ·sv· ·to·
aimpéir | ·ga·
amp | ·ast· ·cy· ·en· ·gd·
narrow-zero | English: ‹{0} A›
{0}A | ·cy·
narrow-one | English: ‹{0}A›
{0} A | ·cs· ·de· ·hr· ·nl· ·tr·
{0}A | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} A›
{0}A | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} A›
{0} A | ·cs· ·hr·
{0}A | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} A›
{0} A | ·cs·
{0}A | ·cy· ·ga·
narrow-other | English: ‹{0}A›
{0} A | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0}A | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
milliampere
long-displayName | English: ‹milliamperes›
mA | ·af· ·am· ·lo· ·ur· ·zu·
mili ampe | ·vi·
miliampea | ·sw·
miliamper | ·sq· ·tr·
miliamperai | ·lt·
miliamperau | ·cy·
miliampere | ·id· ·ms·
miliampereak | ·eu·
miliamperes | ·es_419· ·pt·
miliamperi | ·bs· ·hr· ·ro· ·sl· ·sr_Latn·
miliampēri | ·lv·
miliamperios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
miliamperoù | ·br·
miliampery | ·pl·
miliampéry | ·cs· ·sk·
miliʻamipele | ·to·
mille-ampère | ·gd·
milliampeerit | ·fi·
milliamper | ·az· ·hu· ·is· ·tk· ·uz·
milliampere | ·da· ·it· ·nb· ·sv·
Milliampere | ·de·
milliampère | ·nl·
Milliampère | ·lb·
mil·liampere | ·ca·
milliamperes | ·en· ·fil·
milliampères | ·fr·
milliamperur | ·fo·
milliampery | ·dsb· ·hsb·
milliamprid | ·et·
miollaimpéir | ·ga·
μιλιαμπέρ | ·el·
милиампер | ·mn·
милиампери | ·bg· ·mk· ·sr·
миллиампер | ·kk· ·ky· ·sah·
миллиамперы | ·ru·
міліампери | ·uk·
міліамперы | ·be·
მილიამპერი | ·ka·
միլիամպերներ | ·hy·
מיליאמפר | ·he·
ملي أمبير | ·ar·
میلی‌آمپر | ·fa· ·mzn·
मिलिअँपियर | ·mr·
मिलिएम्पियर | ·ne·
मिली एम्‍पीयर | ·hi·
মিলি-অ্যাম্পিয়ার | ·bn·
ਮਿਲੀਐਮਪੀਅਰ | ·pa·
મિલિએમ્પીયર | ·gu·
மில்லி ஆம்பியர்கள் | ·ta·
మిల్లీ ఆంపియర్స్ | ·te·
ಮಿಲಿಆಂಪೇರ್‌ಗಳು | ·kn·
മില്ലിആമ്പിയർ | ·ml·
මිලි ඇම්පියර | ·si·
มิลลิแอมแปร์ | ·th·
မီလီအမ်ပီယာ | ·my·
មិល្លីអំពែរ | ·km·
ᏌᏉ ᎢᏯᎦᎨᎵᏁᎢ ᏗᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
밀리암페어 | ·ko·
ミリアンペア | ·ja·
毫安 | ·zh·
毫安培 | ·yue· ·zh_Hant·
long-zero | English: ‹{0} mA›
{0} miliamper | ·cy·
{0} miliampēri | ·lv·
{0} ملي أمبير | ·ar·
long-one | English: ‹{0} milliampere›
{0} mA | ·af· ·am· ·ur· ·zu·
{0} mhille-ampère | ·gd·
{0} mhiollaimpéar | ·ga·
{0} miliamper | ·br· ·bs· ·cy· ·hr· ·pl· ·ro· ·sl· ·sq· ·sr_Latn· ·tr·
{0} miliampér | ·cs· ·sk·
{0} miliamperas | ·lt·
{0} miliampere | ·es_419· ·eu· ·pt·
{0} miliamperio | ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
{0} miliampērs | ·lv·
{0} milliampeeri | ·fi·
{0} milliamper | ·az· ·et· ·hu· ·is· ·tk· ·uz·
{0} milliampera | ·fo·
{0} milliampere | ·da· ·dsb· ·en· ·fil· ·hsb· ·it· ·nb· ·sv·
{0} Milliampere | ·de·
{0} milliampère | ·fr· ·nl·
{0} Milliampère | ·lb·
{0} mil·liampere | ·ca·
{0} milliamperiu | ·ast·
{0} μιλιαμπέρ | ·el·
{0} милиампер | ·bg· ·mk· ·mn· ·sr·
{0} миллиампер | ·kk· ·ky· ·ru·
{0} міліампер | ·be· ·uk·
{0} მილიამპერი | ·ka·
{0} միլիամպեր | ·hy·
{0} ملي أمبير | ·ar·
{0} میلی‌آمپر | ·fa·
{0} मिलिअँपियर | ·mr·
{0} मिलिएम्पियर | ·ne·
{0} मिली एम्‍पीयर | ·hi·
{0} মিলি-অ্যাম্পিয়ার | ·bn·
{0} ਮਿਲੀਐਮਪੀਅਰ | ·pa·
{0} મિલિએમ્પીયર | ·gu·
{0} மில்லி ஆம்பியர் | ·ta·
{0} మిల్లీ ఆంపియర్ | ·te·
{0} ಮಿಲಿಆಂಪೇರ್‌ | ·kn·
{0} മില്ലിആമ്പിയർ | ·ml·
{0} ᏌᏉ ᎢᏯᎦᎨᎵᏁᎢ ᎠᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
miliampea {0} | ·sw·
מיליאמפר {0} | ·he·
මිලි ඇම්පියර {0} | ·si·
long-two | English: ‹{0} mA›
{0} filiamper | ·cy·
{0} mhille-ampère | ·gd·
{0} mhiollaimpéar | ·ga·
{0} miliampera | ·sl·
{0} milliampera | ·dsb·
{0} milliamperaj | ·hsb·
{0} viliamper | ·br·
{0} מיליאמפר | ·he·
{0} ملي أمبير | ·ar·
long-few | English: ‹{0} mA›
{0} mhiollaimpéar | ·ga·
{0} miliamper | ·br· ·cy·
{0} miliampera | ·bs· ·hr· ·sr_Latn·
{0} miliamperai | ·lt·
{0} miliamperi | ·ro·
{0} miliampery | ·pl·
{0} miliampéry | ·cs· ·sk·
{0} mille-ampère | ·gd·
{0} milliamperi | ·sl·
{0} milliampery | ·dsb· ·hsb·
{0} милиампера | ·sr·
{0} миллиампера | ·ru·
{0} міліампери | ·uk·
{0} міліамперы | ·be·
{0} ملي أمبير | ·ar·
long-many | English: ‹{0} mA›
{0} a viliamperoù | ·br·
{0} miliamper | ·cy·
{0} miliampéra | ·sk·
{0} miliampero | ·lt·
{0} miliamperów | ·pl·
{0} miliampéru | ·cs·
{0} miollaimpéar | ·ga·
{0} миллиампер | ·ru·
{0} міліампер | ·be·
{0} міліамперів | ·uk·
{0} מיליאמפר | ·he·
{0} ملي أمبير | ·ar·
long-other | English: ‹{0} milliamperes›
{0} de miliamperi | ·ro·
{0} mA | ·af· ·am· ·lo· ·ur· ·zu·
{0} mili ampe | ·vi·
{0} miliamper | ·br· ·cy· ·sq· ·tr·
{0} miliampera | ·bs· ·hr· ·pl· ·sr_Latn·
{0} miliampere | ·eu· ·id· ·ms·
{0} miliamperes | ·es_419· ·pt·
{0} miliampēri | ·lv·
{0} miliamperios | ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY· ·gl·
{0} miliamperov | ·sl·
{0} miliampérov | ·sk·
{0} miliamperų | ·lt·
{0} miliampérů | ·cs·
{0} mille-ampère | ·gd·
{0} milliampeeria | ·fi·
{0} milliamper | ·az· ·hu· ·is· ·tk· ·uz·
{0} milliampere | ·da· ·it· ·nb· ·sv·
{0} Milliampere | ·de·
{0} milliampère | ·nl·
{0} Milliampère | ·lb·
{0} milliamperes | ·en·
{0} milliampères | ·fr·
{0} mil·liamperes | ·ca·
{0} milliamperios | ·ast·
{0} milliamperow | ·dsb· ·hsb·
{0} milliamperur | ·fo·
{0} milliamprit | ·et·
{0} miollaimpéar | ·ga·
{0} na milliampere | ·fil·
{0} μιλιαμπέρ | ·el·
{0} милиампер | ·mn·
{0} милиампера | ·bg· ·sr·
{0} милиампери | ·mk·
{0} миллиампер | ·kk· ·ky· ·sah·
{0} миллиампера | ·ru·
{0} міліампера | ·be· ·uk·
{0} მილიამპერი | ·ka·
{0} միլիամպեր | ·hy·
{0} מיליאמפר | ·he·
{0} ملي أمبير | ·ar·
{0} میلی‌آمپر | ·fa· ·mzn·
{0} मिलिअँपियर | ·mr·
{0} मिलिएम्पियर | ·ne·
{0} मिली एम्‍पीयर | ·hi·
{0} মিলি-অ্যাম্পিয়ার | ·bn·
{0} ਮਿਲੀਐਮਪੀਅਰ | ·pa·
{0} મિલિએમ્પીયર | ·gu·
{0} மில்லி ஆம்பியர்கள் | ·ta·
{0} మిల్లీ ఆంపియర్స్ | ·te·
{0} ಮಿಲಿಆಂಪೇರ್‌ಗಳು | ·kn·
{0} മില്ലിആമ്പിയർ | ·ml·
{0} มิลลิแอมแปร์ | ·th·
{0} မီလီအမ်ပီယာ | ·my·
{0} មិល្លីអំពែរ | ·km·
{0} ᏌᏉ ᎢᏯᎦᎨᎵᏁᎢ ᏗᎾᎦᎵᏍᎩ ᎠᏟᎶᏍᏗ | ·chr·
{0} ミリアンペア | ·ja·
{0} 毫安培 | ·yue· ·zh_Hant·
{0}밀리암페어 | ·ko·
{0}毫安 | ·zh·
miliampea {0} | ·sw·
miliʻamipele ʻe {0} | ·to·
මිලි ඇම්පියරය {0} | ·si·
short-displayName | English: ‹milliamps›
mA | ·all·others·
miliamp | ·id· ·ms·
miliampau | ·cy·
miliampea | ·sw·
miliamper | ·tr·
miliamps | ·ast· ·pt·
mille-amp | ·gd·
milliampere | ·nb·
milliamperur | ·fo·
milliamprid | ·et·
milliamps | ·chr· ·en· ·fil·
miollaimp | ·ga·
μιλιαμπέρ | ·el·
мА | ·be· ·ru· ·uk·
милиамп | ·mn·
милиамп. | ·mk·
миллиамп | ·ky·
миллиампер | ·kk·
მილიამპ. | ·ka·
մԱ | ·hy·
م أمبير | ·ar·
میلی‌آمپر | ·fa· ·mzn·
मि॰ ए॰ | ·hi·
मिलिअँप्स | ·mr·
ਮਿਲੀਐਮਪੀਅਰ | ·pa·
மில்லி ஆம்ப்ஸ் | ·ta·
మిల్లీ ఆంప్స్ | ·te·
ಮಿ.ಆಂ. | ·kn·
മില്ലിആമ്പിയർ | ·ml·
මිලිඇම්පිර | ·si·
มิลลิแอมป์ | ·th·
មិល្លីអំពែរ | ·km·
ミリアンペア | ·ja·
毫安 | ·zh·
毫安培 | ·yue· ·zh_Hant·
short-zero | English: ‹{0} mA›
{0} mA | ·cy· ·lv·
{0} م أمبير | ·ar·
short-one | English: ‹{0} mA›
{0} mA | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·sw· ·tk· ·tr· ·ur· ·uz· ·zu·
{0} мA | ·kk·
{0} мА | ·be· ·ky· ·mn· ·ru· ·uk·
{0} მამპ. | ·ka·
{0} մԱ | ·hy·
{0} م أمبير | ·ar·
{0} میلی‌آمپر | ·fa·
{0} मि॰ ए॰ | ·hi·
{0} மி.ஆ. | ·ta·
{0} మి. ఆం | ·te·
{0} ಮಿ.ಆಂ. | ·kn·
{0} മി.ആ. | ·ml·
මිඇ {0} | ·si·
short-two | English: ‹{0} mA›
{0} mA | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} م أمبير | ·ar·
short-few | English: ‹{0} mA›
{0} mA | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} мА | ·be· ·ru· ·uk·
{0} م أمبير | ·ar·
short-many | English: ‹{0} mA›
{0} mA | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} мА | ·be· ·ru· ·uk·
{0} م أمبير | ·ar·
short-other | English: ‹{0} mA›
{0} mA | ·all·others·
{0} мA | ·kk·
{0} мА | ·be· ·ky· ·mn· ·ru· ·sah· ·uk·
{0} მამპ. | ·ka·
{0} մԱ | ·hy·
{0} م أمبير | ·ar·
{0} میلی‌آمپر | ·fa·
{0} मि॰ ए॰ | ·hi·
{0} மி.ஆ. | ·ta·
{0} మి. ఆం | ·te·
{0} ಮಿ.ಆಂ. | ·kn·
{0} മി.ആ. | ·ml·
{0} มิลลิแอมป์ | ·th·
{0} 毫安培 | ·yue· ·zh_Hant·
{0}mA | ·ko·
{0}毫安 | ·zh·
mA ʻe {0} | ·to·
මිඇ {0} | ·si·
narrow-displayName | English: ‹mA›
mA | ·ast· ·cs· ·cy· ·en· ·fi· ·ga· ·gd· ·sv· ·to·
narrow-zero | English: ‹{0} mA›
{0}mA | ·cy·
narrow-one | English: ‹{0}mA›
{0} mA | ·cs· ·de· ·hr· ·nl· ·tr·
{0}mA | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} mA›
{0}mA | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} mA›
{0} mA | ·cs· ·hr·
{0}mA | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} mA›
{0} mA | ·cs·
{0}mA | ·cy· ·ga·
narrow-other | English: ‹{0}mA›
{0} mA | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0}mA | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
ohm
long-displayName | English: ‹ohms›
ʻōmi | ·to·
ohm | ·af· ·am· ·da· ·dsb· ·fo· ·gd· ·hu· ·id· ·is· ·it· ·lo· ·ms· ·nb· ·ne· ·nl· ·sl· ·sv· ·sw· ·tr· ·ur· ·vi· ·zu·
Ohm | ·de· ·lb·
ohm-ak | ·eu·
ohmau | ·cy·
ohmi | ·ro·
ohmios | ·es· ·es_MX· ·es_US·
ohmit | ·fi·
ohmnios | ·ast·
ohmoù | ·br·
ohms | ·ca· ·en· ·es_419· ·fil· ·fr· ·gl· ·he· ·pt·
ohmy | ·cs· ·hsb· ·sk·
óim | ·ga·
om | ·az· ·sq· ·tk· ·uz·
omai | ·lt·
omi | ·bs· ·hr· ·lv· ·sr_Latn·
omy | ·pl·
oomid | ·et·
ωμ | ·el·
ом | ·ky· ·mn·
Ом | ·kk·
оми | ·mk· ·sr· ·uk·
омове | ·bg·
омы | ·be· ·ru·
ომი | ·ka·
օհմեր | ·hy·
أوم | ·ar·
اهم | ·fa·
اُهم | ·mzn·
ओम | ·hi·
ओहम | ·mr·
ওহম | ·bn·
ਓਹਮ | ·pa·
ઓહ્મ | ·gu·
ஓம்ஸ் | ·ta·
ఓమ్స్ | ·te·
ಓಂಗಳು | ·kn·
ഓം | ·ml·
ඕම් | ·si·
โอห์ม | ·th·
အုမ်း | ·my·
អូម | ·km·
ᏗᎣᎻ | ·chr·
옴 | ·ko·
オーム | ·ja·
欧姆 | ·zh·
歐姆 | ·yue· ·zh_Hant·
long-zero | English: ‹{0} Ω›
{0} ohm | ·cy·
{0} omi | ·lv·
{0} أوم | ·ar·
long-one | English: ‹{0} ohm›
{0} ohm | ·af· ·br· ·ca· ·cs· ·cy· ·da· ·dsb· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·gd· ·gl· ·he· ·hsb· ·hu· ·is· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sv· ·tr·
{0} Ohm | ·lb·
{0} Ohm | ·de·
{0} ohmi | ·fi·
{0} ohmio | ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_MX· ·es_PY· ·es_US·
{0} ohmiu | ·ast·
{0} om | ·az· ·bs· ·hr· ·pl· ·sq· ·sr_Latn· ·tk· ·uz·
{0} óm | ·ga·
{0} omas | ·lt·
{0} oms | ·lv·
{0} oom | ·et·
{0} Ω | ·am· ·ne· ·sw· ·ur· ·zu·
{0} ωμ | ·el·
{0} ом | ·bg· ·ky· ·mk· ·mn· ·ru· ·sr· ·uk·
{0} Ом | ·be· ·kk·
{0} ომი | ·ka·
{0} օհմ | ·hy·
{0} أوم | ·ar·
{0} اهم | ·fa·
{0} ओम | ·hi·
{0} ओहम | ·mr·
{0} ওহম | ·bn·
{0} ਓਹਮ | ·pa·
{0} ઓહ્મ | ·gu·
{0} ஓம் | ·ta·
{0} ఓమ్ | ·te·
{0} ಓಂ | ·kn·
{0} ഓം | ·ml·
{0} ᎣᎻ | ·chr·
ඕම් {0} | ·si·
long-two | English: ‹{0} Ω›
{0} ohm | ·br· ·cy· ·gd·
{0} ohma | ·dsb· ·sl·
{0} ohmaj | ·hsb·
{0} ohms | ·he·
{0} óm | ·ga·
{0} أوم | ·ar·
long-few | English: ‹{0} Ω›
{0} ohm | ·br· ·cy· ·gd·
{0} ohmi | ·ro· ·sl·
{0} ohmy | ·cs· ·dsb· ·hsb· ·sk·
{0} óm | ·ga·
{0} oma | ·bs· ·hr· ·sr_Latn·
{0} omai | ·lt·
{0} omy | ·pl·
{0} Ом | ·be·
{0} ома | ·ru· ·sr·
{0} оми | ·uk·
{0} أوم | ·ar·
long-many | English: ‹{0} Ω›
{0} a ohmoù | ·br·
{0} n-óm | ·ga·
{0} ohm | ·cy·
{0} ohms | ·he·
{0} ohmu | ·cs· ·sk·
{0} omo | ·lt·
{0} omów | ·pl·
{0} ом | ·ru·
{0} Ом | ·be·
{0} омів | ·uk·
{0} أوم | ·ar·
long-other | English: ‹{0} ohms›
{0} de ohmi | ·ro·
{0} na ohm | ·fil·
{0} ohm | ·af· ·br· ·cy· ·da· ·eu· ·fo· ·gd· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·sv· ·tr· ·vi·
{0} Ohm | ·lb·
{0} Ohm | ·de·
{0} ohmia | ·fi·
{0} ohmios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_MX· ·es_PY· ·es_US·
{0} ohmov | ·sk· ·sl·
{0} ohmow | ·dsb· ·hsb·
{0} ohms | ·ca· ·en· ·es_419· ·fr· ·gl· ·he· ·pt·
{0} ohmů | ·cs·
{0} om | ·az· ·sq· ·tk· ·uz·
{0} óm | ·ga·
{0} oma | ·bs· ·hr· ·pl· ·sr_Latn·
{0} omi | ·lv·
{0} omų | ·lt·
{0} oomi | ·et·
{0} Ω | ·am· ·lo· ·mzn· ·ne· ·sw· ·ur· ·zu·
{0} ωμ | ·el·
{0} ом | ·ky· ·mn·
{0} Ом | ·be· ·kk·
{0} ома | ·bg· ·ru· ·sr· ·uk·
{0} оми | ·mk·
{0} ომი | ·ka·
{0} օհմ | ·hy·
{0} أوم | ·ar·
{0} اهم | ·fa·
{0} ओम | ·hi·
{0} ओहम | ·mr·
{0} ওহম | ·bn·
{0} ਓਹਮ | ·pa·
{0} ઓહ્મ | ·gu·
{0} ஓம்ஸ் | ·ta·
{0} ఓమ్స్ | ·te·
{0} ಓಂಗಳು | ·kn·
{0} ഓം | ·ml·
{0} โอห์ม | ·th·
{0} အုမ်း | ·my·
{0} អូម | ·km·
{0} ᏗᎣᎻ | ·chr·
{0} オーム | ·ja·
{0} 歐姆 | ·yue· ·zh_Hant·
{0}옴 | ·ko·
{0}欧姆 | ·zh·
ʻōmi ʻe {0} | ·to·
ඕම් {0} | ·si·
short-displayName | English: ‹ohms›
ohm | ·all·others·
Ohm | ·de·
ohmau | ·cy·
ohmnios | ·ast·
ohms | ·en· ·fil· ·gl· ·he· ·pt·
óim | ·ga·
om | ·az· ·uz·
Om | ·tk·
omi | ·bs·
omy | ·pl·
oomid | ·et·
Ω | ·bg· ·br· ·ca· ·cs· ·da· ·dsb· ·es· ·eu· ·fi· ·fr· ·hr· ·hsb· ·hu· ·it· ·lb· ·lt· ·lv· ·nl· ·ro· ·sk· ·sq· ·sr· ·sr_Latn· ·to· ·vi·
ωμ | ·el·
ом | ·ky· ·mn·
Ом | ·be· ·kk· ·ru·
оми | ·mk· ·uk·
ომი | ·ka·
օմ | ·hy·
أوم | ·ar·
اهم | ·fa· ·mzn·
ओम | ·hi·
ओहम | ·mr·
ওহম | ·bn·
ਓਹਮ | ·pa·
ઓહ્મ | ·gu·
ஓம்ஸ் | ·ta·
ఓమ్స్ | ·te·
ಓಂಗಳು | ·kn·
ഓം | ·ml·
ඕම් | ·si·
โอห์ม | ·th·
အုမ်း | ·my·
អូម | ·km·
ᏗᎣᎻ | ·chr·
オーム | ·ja·
欧姆 | ·zh·
歐姆 | ·yue· ·zh_Hant·
short-zero | English: ‹{0} Ω›
{0} Ω | ·cy· ·lv·
{0} أوم | ·ar·
short-one | English: ‹{0} Ω›
{0} Om | ·tk·
{0} Ω | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·kn· ·ky· ·lb· ·lt· ·lv· ·mk· ·ml· ·mn· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·si· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·sw· ·ta· ·te· ·tr· ·ur· ·uz· ·zu·
{0} Ом | ·be· ·kk· ·ru· ·uk·
{0} ომ | ·ka·
{0} օմ | ·hy·
{0} أوم | ·ar·
{0} اهم | ·fa·
short-two | English: ‹{0} Ω›
{0} Ω | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} أوم | ·ar·
short-few | English: ‹{0} Ω›
{0} Ω | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} Ом | ·be· ·ru· ·uk·
{0} أوم | ·ar·
short-many | English: ‹{0} Ω›
{0} Ω | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} Ом | ·be· ·ru· ·uk·
{0} أوم | ·ar·
short-other | English: ‹{0} Ω›
{0} Om | ·tk·
{0} Ω | ·all·others·
{0} Ом | ·be· ·kk· ·ru· ·uk·
{0} ომ | ·ka·
{0} օմ | ·hy·
{0} أوم | ·ar·
{0} اهم | ·fa·
{0} 歐姆 | ·yue· ·zh_Hant·
{0}Ω | ·ko·
{0}欧 | ·zh·
Ω ʻe {0} | ·to·
narrow-displayName | English: ‹ohm›
ohm | ·cy· ·en· ·gd·
ohmnios | ·ast·
Ω | ·br· ·cs· ·fi· ·ga· ·sv· ·to·
narrow-zero | English: ‹{0} Ω›
{0}Ω | ·cy·
narrow-one | English: ‹{0}Ω›
{0} Ω | ·br· ·cs· ·de· ·hr· ·nl· ·tr·
{0}Ω | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} Ω›
{0} Ω | ·br·
{0}Ω | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} Ω›
{0} Ω | ·br· ·cs· ·hr·
{0}Ω | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} Ω›
{0} Ω | ·br· ·cs·
{0}Ω | ·cy· ·ga·
narrow-other | English: ‹{0}Ω›
{0} Ω | ·br· ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0}Ω | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
volt
long-displayName | English: ‹volts›
foltiau | ·cy·
voldid | ·et·
volotā | ·to·
volt | ·af· ·am· ·az· ·ca· ·da· ·fo· ·gd· ·hu· ·id· ·is· ·it· ·lo· ·ms· ·nb· ·nl· ·sl· ·sq· ·sv· ·tr· ·ur· ·uz· ·zu·
Volt | ·de· ·lb·
voltai | ·lt·
voltak | ·eu·
voltanna | ·ga·
volti | ·bs· ·hr· ·lv· ·sr_Latn· ·sw·
volți | ·ro·
voltios | ·ast· ·es· ·es_MX· ·es_US·
voltit | ·fi·
voltoù | ·br·
volts | ·en· ·es_419· ·fil· ·fr· ·gl· ·pt·
volty | ·cs· ·dsb· ·hsb· ·sk·
vôn | ·vi·
wolt | ·tk·
wolty | ·pl·
βολτ | ·el·
волти | ·mk· ·sr·
волтове | ·bg·
вольт | ·kk· ·ky· ·mn· ·sah·
вольти | ·uk·
вольты | ·be· ·ru·
ვოლტი | ·ka·
վոլտեր | ·hy·
וולט | ·he·
فولت | ·ar·
ولت | ·fa·
وُلت | ·mzn·
भोल्ट | ·ne·
वोल्ट्स | ·hi·
व्होल्ट | ·mr·
ভোল্ট | ·bn·
ਵੋਲਟ | ·pa·
વૉલ્ટ્સ | ·gu·
வோல்ட்கள் | ·ta·
వోల్ట్స్ | ·te·
ವೋಲ್ಟ್‌‌ಗಳು | ·kn·
വോൾട്ട് | ·ml·
වෝල්ට් | ·si·
โวลต์ | ·th·
ဗို့ | ·my·
វ៉ុល | ·km·
ᎠᎾᎦᎵᏍᎩ ᎢᏧᏟᏂᏚᏓ | ·chr·
볼트 | ·ko·
ボルト | ·ja·
伏特 | ·yue· ·zh· ·zh_Hant·
long-zero | English: ‹{0} V›
{0} folt | ·cy·
{0} volti | ·lv·
{0} فولت | ·ar·
long-one | English: ‹{0} volt›
{0} folt | ·cy·
{0} V | ·am· ·ur· ·zu·
{0} volt | ·af· ·az· ·br· ·bs· ·ca· ·cs· ·da· ·dsb· ·en· ·es_419· ·et· ·eu· ·fil· ·fo· ·fr· ·gd· ·gl· ·hr· ·hsb· ·hu· ·is· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr_Latn· ·sv· ·tr· ·uz·
{0} Volt | ·lb·
{0} Volt | ·de·
{0} volta | ·ga·
{0} voltas | ·lt·
{0} voltio | ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_MX· ·es_PY· ·es_US·
{0} voltiu | ·ast·
{0} volts | ·lv·
{0} voltti | ·fi·
{0} wolt | ·pl· ·tk·
{0} βολτ | ·el·
{0} волт | ·bg· ·mk· ·sr·
{0} вольт | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} ვოლტი | ·ka·
{0} վոլտ | ·hy·
{0} فولت | ·ar·
{0} ولت | ·fa·
{0} वोल्ट | ·hi·
{0} व्होल्ट | ·mr·
{0} ভোল্ট | ·bn·
{0} ਵੋਲਟ | ·pa·
{0} વૉલ્ટ્ | ·gu·
{0} வோல்ட் | ·ta·
{0} వోల్ట్ | ·te·
{0} ವೋಲ್ಟ್‌ | ·kn·
{0} വോൾട്ട് | ·ml·
{0} ᎠᎾᎦᎵᏍᎩ ᎢᏳᏟᏂᎩᏓ | ·chr·
{0}भोल्ट | ·ne·
volti {0} | ·sw·
וולט {0} | ·he·
වෝල්ට් {0} | ·si·
long-two | English: ‹{0} V›
{0} folt | ·cy·
{0} volt | ·br· ·gd·
{0} volta | ·dsb· ·ga· ·sl·
{0} voltaj | ·hsb·
{0} וולט | ·he·
{0} فولت | ·ar·
long-few | English: ‹{0} V›
{0} folt | ·cy·
{0} volt | ·br· ·gd·
{0} volta | ·bs· ·ga· ·hr· ·sr_Latn·
{0} voltai | ·lt·
{0} volti | ·sl·
{0} volți | ·ro·
{0} volty | ·cs· ·dsb· ·hsb· ·sk·
{0} wolty | ·pl·
{0} волта | ·sr·
{0} вольта | ·ru·
{0} вольти | ·uk·
{0} вольты | ·be·
{0} فولت | ·ar·
long-many | English: ‹{0} V›
{0} a voltoù | ·br·
{0} folt | ·cy·
{0} volta | ·ga·
{0} volto | ·lt·
{0} voltu | ·cs· ·sk·
{0} woltów | ·pl·
{0} вольт | ·be· ·ru·
{0} вольтів | ·uk·
{0} וולט | ·he·
{0} فولت | ·ar·
long-other | English: ‹{0} volts›
{0} de volți | ·ro·
{0} folt | ·cy·
{0} na volt | ·fil·
{0} V | ·am· ·lo· ·ur· ·zu·
{0} volt | ·af· ·az· ·br· ·da· ·eu· ·fo· ·gd· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·sq· ·sv· ·tr· ·uz·
{0} Volt | ·lb·
{0} Volt | ·de·
{0} volta | ·bs· ·ga·
{0} volti | ·et· ·hr· ·lv· ·sr_Latn·
{0} voltios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_MX· ·es_PY· ·es_US·
{0} voltov | ·sk· ·sl·
{0} voltow | ·dsb· ·hsb·
{0} volts | ·ca· ·en· ·es_419· ·fr· ·gl· ·pt·
{0} volttia | ·fi·
{0} voltů | ·cs·
{0} voltų | ·lt·
{0} vôn | ·vi·
{0} wolt | ·tk·
{0} wolta | ·pl·
{0} βολτ | ·el·
{0} волта | ·bg·
{0} волти | ·mk· ·sr·
{0} вольт | ·kk· ·ky· ·mn·
{0} вольта | ·be· ·ru· ·uk·
{0} ვოლტი | ·ka·
{0} վոլտ | ·hy·
{0} וולט | ·he·
{0} فولت | ·ar·
{0} ولت | ·fa· ·mzn·
{0} वोल्ट्स | ·hi·
{0} व्होल्ट | ·mr·
{0} ভোল্ট | ·bn·
{0} ਵੋਲਟ | ·pa·
{0} વૉલ્ટ્ | ·gu·
{0} வோல்ட்கள் | ·ta·
{0} వోల్ట్స్ | ·te·
{0} ವೋಲ್ಟ್‌ಗಳು | ·kn·
{0} വോൾട്ട് | ·ml·
{0} โวลต์ | ·th·
{0} ဗို့ | ·my·
{0} វ៉ុល | ·km·
{0} ᎠᎾᎦᎵᏍᎩ ᎢᏧᏟᏂᏚᏓ | ·chr·
{0} ボルト | ·ja·
{0} 伏特 | ·yue· ·zh_Hant·
{0}भोल्ट | ·ne·
{0}볼트 | ·ko·
{0}伏特 | ·zh·
volotā ʻe {0} | ·to·
volti {0} | ·sw·
වෝල්ට් {0} | ·si·
short-displayName | English: ‹volts›
foltiau | ·cy·
v | ·vi·
V | ·bg· ·br· ·ca· ·cs· ·da· ·dsb· ·eu· ·fi· ·fr· ·hr· ·hsb· ·hu· ·it· ·lb· ·lt· ·lv· ·nl· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn·
voldid | ·et·
volotā | ·to·
volt | ·all·others·
Volt | ·de·
voltanna | ·ga·
volti | ·bs· ·sw·
voltios | ·ast· ·es· ·es_AR· ·es_CL· ·es_DO· ·es_GT· ·es_PY·
volts | ·en· ·es_419· ·fil· ·gl· ·pt·
W | ·tk·
wolty | ·pl·
βολτ | ·el·
В | ·be· ·ru·
волти | ·mk·
вольт | ·kk· ·ky· ·mn·
вольти | ·uk·
ვოლტი | ·ka·
Վ | ·hy·
וולט | ·he·
فولت | ·ar·
ولت | ·fa· ·mzn·
भोल्ट | ·ne·
वोल्ट | ·hi·
व्होल्ट | ·mr·
ভোল্ট | ·bn·
ਵੋਲਟ | ·pa·
வோ. | ·ta·
వోల్ట్స్ | ·te·
ವೋ. | ·kn·
വോൾട്ട് | ·ml·
වෝල්ට් | ·si·
โวลต์ | ·th·
ဗို့ | ·my·
វ៉ុល | ·km·
ᎠᎾᎦᎵᏍᎩ ᎢᏧᏟᏂᏚᏓ | ·chr·
ボルト | ·ja·
伏特 | ·yue· ·zh· ·zh_Hant·
short-zero | English: ‹{0} V›
{0} V | ·cy· ·lv·
{0} فولت | ·ar·
short-one | English: ‹{0} V›
{0} V | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·ml· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tr· ·ur· ·uz· ·zu·
{0} W | ·tk·
{0} В | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} ვ | ·ka·
{0} Վ | ·hy·
{0} فولت | ·ar·
{0} ولت | ·fa·
{0} வோ. | ·ta·
{0} వో | ·te·
{0} ವೋ | ·kn·
volti {0} | ·sw·
වෝ {0} | ·si·
short-two | English: ‹{0} V›
{0} V | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} فولت | ·ar·
short-few | English: ‹{0} V›
{0} V | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} В | ·be· ·ru· ·uk·
{0} فولت | ·ar·
short-many | English: ‹{0} V›
{0} V | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} В | ·be· ·ru· ·uk·
{0} فولت | ·ar·
short-other | English: ‹{0} V›
{0} V | ·all·others·
{0} W | ·tk·
{0} В | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} ვ | ·ka·
{0} Վ | ·hy·
{0} فولت | ·ar·
{0} ولت | ·fa·
{0} வோ. | ·ta·
{0} వో | ·te·
{0} ವೋ. | ·kn·
{0} 伏 | ·yue· ·zh_Hant·
{0} 伏特 | ·zh_Hant_HK·
{0}V | ·ko·
{0}伏 | ·zh·
V ʻe {0} | ·to·
volti {0} | ·sw·
වෝ {0} | ·si·
narrow-displayName | English: ‹volt›
folt | ·cy·
V | ·cs· ·fi· ·sv· ·to·
volt | ·en· ·gd·
volta | ·ga·
volti | ·sw·
voltios | ·ast·
narrow-zero | English: ‹{0} V›
{0}V | ·cy·
narrow-one | English: ‹{0}V›
{0} V | ·cs· ·de· ·hr· ·nl· ·tr·
{0}V | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} V›
{0}V | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} V›
{0} V | ·cs· ·hr·
{0}V | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} V›
{0} V | ·cs·
{0}V | ·cy· ·ga·
narrow-other | English: ‹{0}V›
{0} V | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0}V | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
gigahertz
long-displayName | English: ‹gigahertz›
GHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
giga-hertz | ·gd·
gigagers | ·uz·
gigagerts | ·tk·
gigaherc | ·sq·
gigahercai | ·lt·
gigaherce | ·pl·
gigaherci | ·bs· ·hr· ·lv· ·sr_Latn·
gigahercios | ·ast· ·es·
gigaherts | ·cy·
gigahertsid | ·et·
gigahertsit | ·fi·
gigahertz | ·ca· ·da· ·en· ·eu· ·fil· ·fo· ·fr· ·hu· ·id· ·it· ·ms· ·nb· ·nl· ·pt· ·ro· ·sl· ·sv· ·tr·
Gigahertz | ·de· ·lb·
gígahertz | ·is·
gigahertze | ·sk·
gigahertzoù | ·br·
gigahertzy | ·cs· ·dsb· ·hsb·
gigahezi | ·sw·
gigiheirts | ·ga·
giqahers | ·az·
kikahēti | ·to·
xigahertz | ·gl·
γιγαχέρτζ | ·el·
гигагерц | ·kk· ·ky· ·mn·
гигагерцы | ·ru·
гигахерц | ·mk·
гигахерци | ·bg· ·sr·
гігагерци | ·uk·
гігагерцы | ·be·
გიგაჰერცი | ·ka·
գիգահերցեր | ·hy·
ג׳יגה-הרץ | ·he·
غيغا هرتز | ·ar·
گیگاهرتز | ·fa· ·mzn·
गिगाहर्ज | ·ne·
गिगाहर्ट्झ | ·mr·
गीगाहर्ट्ज़ | ·hi·
গিগাহার্জ | ·bn·
ਗੀਗਾਹਰਟਜ਼ | ·pa·
ગીગાહર્ટ્ઝ | ·gu·
கிகாஹெர்ட்ஸ் | ·ta·
గిగాహెర్ట్‌జ్ | ·te·
ಗಿಗಾಹರ್ಟ್ಸ್‌ | ·kn·
ജിഗാഹെർട്സ് | ·ml·
ගිගාහට්ස් | ·si·
กิกะเฮิรตซ์ | ·th·
ဂီဂါဟတ်ဇ် | ·my·
ជីកាហឺត | ·km·
ᎩᎦᎭᏥ | ·chr·
기가헤르츠 | ·ko·
ギガヘルツ | ·ja·
吉赫 | ·yue· ·zh· ·zh_Hant·
long-zero | English: ‹{0} GHz›
{0} gigaherci | ·lv·
{0} gigaherts | ·cy·
{0} غيغا هرتز | ·ar·
long-one | English: ‹{0} gigahertz›
{0} ghiga-hertz | ·gd·
{0} ghigiheirts | ·ga·
{0} GHz | ·af· ·am· ·ur· ·zu·
{0} gigagers | ·uz·
{0} gigagerts | ·tk·
{0} gigaherc | ·bs· ·hr· ·pl· ·sq· ·sr_Latn·
{0} gigahercas | ·lt·
{0} gigahercio | ·es· ·es_MX· ·es_US·
{0} gigaherciu | ·ast·
{0} gigahercs | ·lv·
{0} gigaherts | ·cy· ·et·
{0} gigahertsi | ·fi·
{0} gigahertz | ·br· ·ca· ·cs· ·da· ·dsb· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·hsb· ·hu· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sv· ·tr·
{0} Gigahertz | ·lb·
{0} Gigahertz | ·de·
{0} gígahertz | ·is·
{0} giqahers | ·az·
{0} xigahertz | ·gl·
{0} γιγαχέρτζ | ·el·
{0} гигагерц | ·kk· ·ky· ·mn· ·ru·
{0} гигахерц | ·bg· ·mk· ·sr·
{0} гігагерц | ·be· ·uk·
{0} გიგაჰერცი | ·ka·
{0} գիգահերց | ·hy·
{0} غيغا هرتز | ·ar·
{0} گیگاهرتز | ·fa·
{0} गिगाहर्ट्झ | ·mr·
{0} गीगाहर्ट्ज़ | ·hi·
{0} গিগাহার্জ | ·bn·
{0} ਗੀਗਾਹਰਟਜ਼ | ·pa·
{0} ગીગાહર્ટ્ઝ | ·gu·
{0} கிகாஹெர்ட்ஸ் | ·ta·
{0} గిగాహెర్ట్‌జ్ | ·te·
{0} ಗಿಗಾಹರ್ಟ್ಸ್‌ | ·kn·
{0} ജിഗാഹെർട്സ് | ·ml·
{0} ᎩᎦᎭᏥ | ·chr·
{0}गिगाहर्ज | ·ne·
gigahezi {0} | ·sw·
ג׳יגה-הרץ {0} | ·he·
ගිගාහට්ස් {0} | ·si·
long-two | English: ‹{0} GHz›
{0} c'higahertz | ·br·
{0} ghiga-hertz | ·gd·
{0} ghigiheirts | ·ga·
{0} gigaherts | ·cy·
{0} gigahertza | ·dsb· ·sl·
{0} gigahertzaj | ·hsb·
{0} ג׳יגה-הרץ | ·he·
{0} غيغا هرتز | ·ar·
long-few | English: ‹{0} GHz›
{0} ghigiheirts | ·ga·
{0} giga-hertz | ·gd·
{0} gigaherca | ·bs· ·hr· ·sr_Latn·
{0} gigahercai | ·lt·
{0} gigaherce | ·pl·
{0} gigaherts | ·cy·
{0} gigahertz | ·br·
{0} gigahertze | ·sk·
{0} gigahertzi | ·ro· ·sl·
{0} gigahertzy | ·cs· ·dsb· ·hsb·
{0} гигагерца | ·ru·
{0} гигахерца | ·sr·
{0} гігагерци | ·uk·
{0} гігагерцы | ·be·
{0} غيغا هرتز | ·ar·
long-many | English: ‹{0} GHz›
{0} a c'higahertzoù | ·br·
{0} gigaherco | ·lt·
{0} gigaherców | ·pl·
{0} gigaherts | ·cy·
{0} gigahertza | ·sk·
{0} gigahertzu | ·cs·
{0} ngigiheirts | ·ga·
{0} гигагерц | ·ru·
{0} гігагерц | ·be·
{0} гігагерців | ·uk·
{0} ג׳יגה-הרץ | ·he·
{0} غيغا هرتز | ·ar·
long-other | English: ‹{0} gigahertz›
{0} de gigahertzi | ·ro·
{0} GHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
{0} giga-hertz | ·gd·
{0} gigagers | ·uz·
{0} gigagerts | ·tk·
{0} gigaherc | ·sq·
{0} gigaherca | ·bs· ·hr· ·pl· ·sr_Latn·
{0} gigaherci | ·lv·
{0} gigahercios | ·ast· ·es· ·es_MX· ·es_US·
{0} gigahercų | ·lt·
{0} gigaherts | ·cy·
{0} gigahertsi | ·et·
{0} gigahertsiä | ·fi·
{0} gigahertz | ·br· ·da· ·en· ·es_419· ·eu· ·fo· ·fr· ·hu· ·id· ·it· ·ms· ·nb· ·nl· ·pt· ·sv· ·tr·
{0} Gigahertz | ·lb·
{0} Gigahertz | ·de·
{0} gígahertz | ·is·
{0} gigahertzev | ·sl·
{0} gigahertzov | ·sk·
{0} gigahertzow | ·dsb· ·hsb·
{0} gigahertzs | ·ca·
{0} gigahertzů | ·cs·
{0} gigiheirts | ·ga·
{0} giqahers | ·az·
{0} na gigahertz | ·fil·
{0} xigahertz | ·gl·
{0} γιγαχέρτζ | ·el·
{0} гигагерц | ·kk· ·ky· ·mn·
{0} гигагерца | ·ru·
{0} гигахерца | ·bg· ·sr·
{0} гигахерци | ·mk·
{0} гігагерца | ·be· ·uk·
{0} გიგაჰერცი | ·ka·
{0} գիգահերց | ·hy·
{0} ג׳יגה-הרץ | ·he·
{0} غيغا هرتز | ·ar·
{0} گیگاهرتز | ·fa· ·mzn·
{0} गिगाहर्ट्झ | ·mr·
{0} गीगाहर्ट्ज़ | ·hi·
{0} গিগাহার্জ | ·bn·
{0} ਗੀਗਾਹਰਟਜ਼ | ·pa·
{0} ગીગાહર્ટ્ઝ | ·gu·
{0} கிகாஹெர்ட்ஸ் | ·ta·
{0} గిగాహెర్ట్‌జ్ | ·te·
{0} ಗಿಗಾಹರ್ಟ್ಸ್‌ | ·kn·
{0} ജിഗാഹെർട്സ് | ·ml·
{0} กิกะเฮิรตซ์ | ·th·
{0} ဂီဂါဟတ်ဇ် | ·my·
{0} ជីកាហឺត | ·km·
{0} ᎩᎦᎭᏥ | ·chr·
{0} ギガヘルツ | ·ja·
{0} 吉赫 | ·yue· ·zh_Hant·
{0}गिगाहर्ज | ·ne·
{0}기가헤르츠 | ·ko·
{0}吉赫 | ·zh·
gigahezi {0} | ·sw·
kikahēti ʻe {0} | ·to·
ගිගාහට්ස් {0} | ·si·
short-displayName | English: ‹GHz›
GGs | ·tk· ·uz·
GHz | ·all·others·
gigahezi | ·sw·
γιγαχέρτζ | ·el·
Ггц | ·ky·
ГГц | ·be· ·kk· ·mn· ·ru· ·uk·
გჰც. | ·ka·
ԳՀց | ·hy·
غ هرتز | ·ar·
گیگاهرتز | ·fa· ·mzn·
ஜி.ஹெஸ். | ·ta·
గిగా హె | ·te·
ಗಿ.ಹ | ·kn·
ജി.ഹെ. | ·ml·
ගිහස් | ·si·
ဂီဂါဟတ်ဇ် | ·my·
吉赫 | ·yue· ·zh· ·zh_Hant·
short-zero | English: ‹{0} GHz›
{0} GHz | ·cy· ·lv·
{0} غ هرتز | ·ar·
short-one | English: ‹{0} GHz›
{0} GGs | ·tk· ·uz·
{0} GHz | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tr· ·ur· ·zu·
{0} Ггц | ·ky·
{0} ГГц | ·be· ·kk· ·mn· ·ru· ·uk·
{0} გჰც. | ·ka·
{0} ԳՀց | ·hy·
{0} غ هرتز | ·ar·
{0} گیگاهرتز | ·fa·
{0} ஜி.ஹெஸ். | ·ta·
{0} గిగా హె | ·te·
{0} ಗಿ.ಹ | ·kn·
{0} ജി.ഹെ. | ·ml·
gigahezi {0} | ·sw·
ගිහස් {0} | ·si·
short-two | English: ‹{0} GHz›
{0} GHz | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} غ هرتز | ·ar·
short-few | English: ‹{0} GHz›
{0} GHz | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} ГГц | ·be· ·ru· ·uk·
{0} غ هرتز | ·ar·
short-many | English: ‹{0} GHz›
{0} GHz | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} ГГц | ·be· ·ru· ·uk·
{0} غ هرتز | ·ar·
short-other | English: ‹{0} GHz›
{0} GGs | ·tk· ·uz·
{0} GHz | ·all·others·
{0} Ггц | ·ky·
{0} ГГц | ·be· ·kk· ·mn· ·ru· ·uk·
{0} გჰც. | ·ka·
{0} ԳՀց | ·hy·
{0} غ هرتز | ·ar·
{0} گیگاهرتز | ·fa·
{0} ஜி.ஹெஸ். | ·ta·
{0} గిగా హె | ·te·
{0} ಗಿ.ಹ | ·kn·
{0} ജി.ഹെ. | ·ml·
{0} 吉赫 | ·yue· ·zh_Hant·
{0}GHz | ·ko·
{0}吉赫 | ·zh·
GHz ʻe {0} | ·to·
gigahezi {0} | ·sw·
ගිහස් {0} | ·si·
narrow-displayName | English: ‹GHz›
GHz | ·ast· ·cs· ·cy· ·en· ·fi· ·ga· ·gd· ·sv· ·to·
گ‌.هرتز | ·fa·
narrow-zero | English: ‹{0} GHz›
{0}GHz | ·cy·
narrow-one | English: ‹{0}GHz›
{0} GHz | ·cs· ·de· ·hr· ·nl· ·tr·
{0} گ.هرتز | ·fa·
{0}GHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} GHz›
{0}GHz | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} GHz›
{0} GHz | ·cs· ·hr·
{0}GHz | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} GHz›
{0} GHz | ·cs·
{0}GHz | ·cy· ·ga·
narrow-other | English: ‹{0}GHz›
{0} GHz | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0} گ.هرتز | ·fa·
{0}GHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
megahertz
long-displayName | English: ‹megahertz›
meaga-hertz | ·gd·
megagers | ·uz·
megagerts | ·tk·
megaherc | ·sq·
megahercai | ·lt·
megaherce | ·pl·
megaherci | ·bs· ·hr· ·lv· ·sr_Latn·
megahercios | ·ast· ·es· ·es_MX· ·es_US·
megaherts | ·cy·
megahertsid | ·et·
megahertsit | ·fi·
megahertz | ·ca· ·da· ·en· ·es_419· ·eu· ·fil· ·fo· ·gl· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·pt· ·ro· ·sl· ·sv· ·tr·
Megahertz | ·de· ·lb·
mégahertz | ·fr·
megahertze | ·sk·
megahertzoù | ·br·
megahertzy | ·cs· ·dsb· ·hsb·
megahēti | ·to·
megahezi | ·sw·
meigiheirts | ·ga·
meqahers | ·az·
MHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
μεγαχέρτζ | ·el·
мегагерц | ·kk· ·ky· ·mn·
мегагерци | ·uk·
мегагерцы | ·be· ·ru·
мегахерц | ·mk·
мегахерци | ·bg· ·sr·
მეგაჰერცი | ·ka·
մեգահերցեր | ·hy·
מגה-הרץ | ·he·
مگاهرتز | ·fa· ·mzn·
ميغا هرتز | ·ar·
मेगाहर्ज | ·ne·
मेगाहर्ट्ज़ | ·hi·
मेगाहर्ट्झ | ·mr·
মেগাহার্জ | ·bn·
ਮੈਗਾਹਰਟਜ਼ | ·pa·
મેગાહર્ટ્ઝ | ·gu·
மெகாஹெர்ட்ஸ் | ·ta·
మెగాహెర్ట్‌జ్ | ·te·
ಮೆಗಾಹರ್ಟ್ಸ್ | ·kn·
മെഗാഹെർട്സ് | ·ml·
මෙගාහර්ට්ස් | ·si·
เมกะเฮิรตซ์ | ·th·
မီဂါဟတ်ဇ် | ·my·
មេហ្គា​ហឺត | ·km·
ᎺᎦᎭᏥ | ·chr·
메가헤르츠 | ·ko·
メガヘルツ | ·ja·
兆赫 | ·yue· ·zh· ·zh_Hant·
long-zero | English: ‹{0} MHz›
{0} megaherci | ·lv·
{0} megaherts | ·cy·
{0} ميغا هرتز | ·ar·
long-one | English: ‹{0} megahertz›
{0} megagers | ·uz·
{0} megagerts | ·tk·
{0} megaherc | ·bs· ·hr· ·pl· ·sq· ·sr_Latn·
{0} megahercas | ·lt·
{0} megahercio | ·es· ·es_MX· ·es_US·
{0} megaherciu | ·ast·
{0} megahercs | ·lv·
{0} megaherts | ·cy· ·et·
{0} megahertsi | ·fi·
{0} megahertz | ·br· ·ca· ·cs· ·da· ·dsb· ·en· ·es_419· ·eu· ·fo· ·gl· ·hsb· ·hu· ·is· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sv· ·tr·
{0} Megahertz | ·lb·
{0} Megahertz | ·de·
{0} mégahertz | ·fr·
{0} meqahers | ·az·
{0} mheaga-hertz | ·gd·
{0} mheigiheirts | ·ga·
{0} MHz | ·af· ·am· ·ur· ·zu·
{0} na megahertz | ·fil·
{0} μεγαχέρτζ | ·el·
{0} мегагерц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} мегахерц | ·bg· ·mk· ·sr·
{0} მეგაჰერცი | ·ka·
{0} մեգահերց | ·hy·
{0} مگاهرتز | ·fa·
{0} ميغا هرتز | ·ar·
{0} मेगाहर्ज | ·ne·
{0} मेगाहर्ट्ज़ | ·hi·
{0} मेगाहर्ट्झ | ·mr·
{0} মেগাহার্জ | ·bn·
{0} ਮੈਗਾਹਰਟਜ਼ | ·pa·
{0} મેગાહર્ટ્ઝ | ·gu·
{0} மெகாஹெர்ட்ஸ் | ·ta·
{0} మెగాహెర్ట్‌జ్ | ·te·
{0} ಮೆಗಾಹರ್ಟ್ಸ್ | ·kn·
{0} മെഗാഹെർട്സ് | ·ml·
{0} ᎺᎦᎭᏥ | ·chr·
megahezi {0} | ·sw·
מגה-הרץ {0} | ·he·
මෙගාහර්ට්ස් {0} | ·si·
long-two | English: ‹{0} MHz›
{0} fegaherts | ·cy·
{0} megahertza | ·dsb· ·sl·
{0} megahertzaj | ·hsb·
{0} mheaga-hertz | ·gd·
{0} mheigiheirts | ·ga·
{0} vegahertz | ·br·
{0} מגה-הרץ | ·he·
{0} ميغا هرتز | ·ar·
long-few | English: ‹{0} MHz›
{0} meaga-hertz | ·gd·
{0} megaherca | ·bs· ·hr· ·sr_Latn·
{0} megahercai | ·lt·
{0} megaherce | ·pl·
{0} megaherts | ·cy·
{0} megahertz | ·br·
{0} megahertze | ·sk·
{0} megahertzi | ·ro· ·sl·
{0} megahertzy | ·cs· ·dsb· ·hsb·
{0} mheigiheirts | ·ga·
{0} мегагерца | ·ru·
{0} мегагерци | ·uk·
{0} мегагерцы | ·be·
{0} мегахерца | ·sr·
{0} ميغا هرتز | ·ar·
long-many | English: ‹{0} MHz›
{0} a vegahertzoù | ·br·
{0} megaherco | ·lt·
{0} megaherców | ·pl·
{0} megaherts | ·cy·
{0} megahertza | ·sk·
{0} megahertzu | ·cs·
{0} meigiheirts | ·ga·
{0} мегагерц | ·be· ·ru·
{0} мегагерців | ·uk·
{0} מגה-הרץ | ·he·
{0} ميغا هرتز | ·ar·
long-other | English: ‹{0} megahertz›
{0} de megahertzi | ·ro·
{0} meaga-hertz | ·gd·
{0} megagers | ·uz·
{0} megagerts | ·tk·
{0} megaherc | ·sq·
{0} megaherca | ·bs· ·hr· ·pl· ·sr_Latn·
{0} megaherci | ·lv·
{0} megahercios | ·ast· ·es· ·es_MX· ·es_US·
{0} megahercų | ·lt·
{0} megaherts | ·cy·
{0} megahertsi | ·et·
{0} megahertsiä | ·fi·
{0} megahertz | ·br· ·da· ·en· ·es_419· ·eu· ·fil· ·fo· ·gl· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·pt· ·sv· ·tr·
{0} Megahertz | ·lb·
{0} Megahertz | ·de·
{0} mégahertz | ·fr·
{0} megahertzev | ·sl·
{0} megahertzov | ·sk·
{0} megahertzow | ·dsb· ·hsb·
{0} megahertzs | ·ca·
{0} megahertzů | ·cs·
{0} meigiheirts | ·ga·
{0} meqahers | ·az·
{0} MHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
{0} μεγαχέρτζ | ·el·
{0} мегагерц | ·kk· ·ky· ·mn·
{0} мегагерца | ·be· ·ru· ·uk·
{0} мегахерца | ·bg· ·sr·
{0} мегахерци | ·mk·
{0} მეგაჰერცი | ·ka·
{0} մեգահերց | ·hy·
{0} מגה-הרץ | ·he·
{0} مگاهرتز | ·fa· ·mzn·
{0} ميغا هرتز | ·ar·
{0} मेगाहर्ज | ·ne·
{0} मेगाहर्ट्ज़ | ·hi·
{0} मेगाहर्ट्झ | ·mr·
{0} মেগাহার্জ | ·bn·
{0} ਮੈਗਾਹਰਟਜ਼ | ·pa·
{0} મેગાહર્ટ્ઝ | ·gu·
{0} மெகாஹெர்ட்ஸ் | ·ta·
{0} మెగాహెర్ట్‌జ్ | ·te·
{0} ಮೆಗಾಹರ್ಟ್ಸ್ | ·kn·
{0} മെഗാഹെർട്സ് | ·ml·
{0} เมกะเฮิรตซ์ | ·th·
{0} မီဂါဟတ်ဇ် | ·my·
{0} មេហ្គា​ហឺត | ·km·
{0} ᎺᎦᎭᏥ | ·chr·
{0} メガヘルツ | ·ja·
{0} 兆赫 | ·yue· ·zh_Hant·
{0}메가헤르츠 | ·ko·
{0}兆赫 | ·zh·
megahēti ʻe {0} | ·to·
megahezi {0} | ·sw·
මෙගාහර්ට්ස් {0} | ·si·
short-displayName | English: ‹MHz›
megahezi | ·sw·
MGs | ·tk· ·uz·
MHz | ·all·others·
μεγαχέρτζ | ·el·
МГц | ·be· ·kk· ·mn· ·ru· ·uk·
МГЦ | ·ky·
მჰც | ·ka·
ՄՀց | ·hy·
م هرتز | ·ar·
مگاهرتز | ·fa· ·mzn·
மெ.ஹெஸ். | ·ta·
మె.హె | ·te·
ಮೆ.ಹ | ·kn·
മെ.ഹെ. | ·ml·
මෙග | ·si·
မီဂါဟတ်ဇ် | ·my·
兆赫 | ·yue· ·zh· ·zh_Hant·
short-zero | English: ‹{0} MHz›
{0} MHz | ·cy· ·lv·
{0} م هرتز | ·ar·
short-one | English: ‹{0} MHz›
{0} MGs | ·tk· ·uz·
{0} MHz | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tr· ·ur· ·zu·
{0} MГц | ·kk·
{0} МГц | ·be· ·mn· ·ru· ·uk·
{0} МГЦ | ·ky·
{0} მჰც | ·ka·
{0} ՄՀց | ·hy·
{0} م هرتز | ·ar·
{0} مگاهرتز | ·fa·
{0} மெ.ஹெஸ். | ·ta·
{0} మె.హె | ·te·
{0} ಮೆ.ಹ | ·kn·
{0} മെ.ഹെ. | ·ml·
megahezi {0} | ·sw·
මෙහ {0} | ·si·
short-two | English: ‹{0} MHz›
{0} MHz | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} م هرتز | ·ar·
short-few | English: ‹{0} MHz›
{0} MHz | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} МГц | ·be· ·ru· ·uk·
{0} م هرتز | ·ar·
short-many | English: ‹{0} MHz›
{0} MHz | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} МГц | ·be· ·ru· ·uk·
{0} م هرتز | ·ar·
short-other | English: ‹{0} MHz›
{0} MGs | ·tk· ·uz·
{0} MHz | ·all·others·
{0} MГц | ·kk·
{0} МГц | ·be· ·mn· ·ru· ·uk·
{0} МГЦ | ·ky·
{0} მჰც | ·ka·
{0} ՄՀց | ·hy·
{0} م هرتز | ·ar·
{0} مگاهرتز | ·fa·
{0} மெ.ஹெஸ். | ·ta·
{0} మె.హె | ·te·
{0} ಮೆ.ಹ | ·kn·
{0} മെ.ഹെ. | ·ml·
{0} 兆赫 | ·yue· ·zh_Hant·
{0}MHz | ·ko·
{0}兆赫 | ·zh·
megahezi {0} | ·sw·
MHz ʻe {0} | ·to·
මෙහ {0} | ·si·
narrow-displayName | English: ‹MHz›
MHz | ·ast· ·cs· ·cy· ·en· ·fi· ·ga· ·gd· ·sv· ·to·
مگاهرتز | ·fa·
narrow-zero | English: ‹{0} MHz›
{0}MHz | ·cy·
narrow-one | English: ‹{0}MHz›
{0} MHz | ·cs· ·de· ·hr· ·nl· ·tr·
{0} مگاهرتز | ·fa·
{0}MHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} MHz›
{0}MHz | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} MHz›
{0} MHz | ·cs· ·hr·
{0}MHz | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} MHz›
{0} MHz | ·cs·
{0}MHz | ·cy· ·ga·
narrow-other | English: ‹{0}MHz›
{0} MHz | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0} مگاهرتز | ·fa·
{0}MHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
kilohertz
long-displayName | English: ‹kilohertz›
cile-hertz | ·gd·
ciliheirts | ·ga·
ciloherts | ·cy·
kHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
kilogers | ·uz·
kilogerts | ·tk·
kiloherc | ·sq·
kilohercai | ·lt·
kiloherce | ·pl·
kiloherci | ·bs· ·hr· ·lv· ·sr_Latn·
kilohercios | ·es· ·es_MX· ·es_US·
kilohers | ·az·
kilohertsid | ·et·
kilohertsit | ·fi·
kilohertz | ·da· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·gl· ·hu· ·id· ·it· ·ms· ·nb· ·nl· ·pt· ·ro· ·sl· ·sv· ·tr·
Kilohertz | ·de· ·lb·
kílóhertz | ·is·
kilohertze | ·sk·
kilohertzoù | ·br·
kilohertzy | ·cs· ·dsb· ·hsb·
kilohēti | ·to·
kilohezi | ·sw·
quilohercios | ·ast·
quilohertz | ·ca·
κιλοχέρτζ | ·el·
килогерц | ·kk· ·ky· ·mn·
килогерцы | ·ru·
килохерц | ·mk·
килохерци | ·bg· ·sr·
кілагерцы | ·be·
кілогерци | ·uk·
კილოჰერცი | ·ka·
կիլոհերցեր | ·hy·
קילו-הרץ | ·he·
كيلو هرتز | ·ar·
کیلوهرتز | ·fa· ·mzn·
किलोहर्ज | ·ne·
किलोहर्ट्ज़ | ·hi·
किलोहर्ट्झ | ·mr·
কিলোহার্জ | ·bn·
ਕਿਲੋਹਰਟਜ਼ | ·pa·
કિલોહર્ટ્ઝ | ·gu·
கிலோஹெர்ட்ஸ் | ·ta·
కిలోహెర్ట్‌జ్ | ·te·
ಕಿಲೋಹರ್ಟ್ಸ್‌ | ·kn·
കിലോഹെർട്സ് | ·ml·
කිලෝහට්ස් | ·si·
กิโลเฮิรตซ์ | ·th·
ကီလိုဟတ်ဇ် | ·my·
គីឡូហឺត | ·km·
ᎠᎦᏴᎵᎭᏥ | ·chr·
킬로헤르츠 | ·ko·
キロヘルツ | ·ja·
千赫 | ·yue· ·zh· ·zh_Hant·
long-zero | English: ‹{0} kHz›
{0} ciloherts | ·cy·
{0} kiloherci | ·lv·
{0} كيلو هرتز | ·ar·
long-one | English: ‹{0} kilohertz›
{0} c'hilohertz | ·br·
{0} chile-hertz | ·gd·
{0} chiliheirts | ·ga·
{0} ciloherts | ·cy·
{0} kHz | ·af· ·am· ·ur· ·zu·
{0} kilogers | ·uz·
{0} kilogerts | ·tk·
{0} kiloherc | ·bs· ·hr· ·pl· ·sq· ·sr_Latn·
{0} kilohercas | ·lt·
{0} kilohercio | ·es· ·es_MX· ·es_US·
{0} kilohercs | ·lv·
{0} kilohers | ·az·
{0} kiloherts | ·et·
{0} kilohertsi | ·fi·
{0} kilohertz | ·cs· ·da· ·dsb· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·gl· ·hsb· ·hu· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sv· ·tr·
{0} Kilohertz | ·lb·
{0} Kilohertz | ·de·
{0} kílóhertz | ·is·
{0} quiloherciu | ·ast·
{0} quilohertz | ·ca·
{0} κιλοχέρτζ | ·el·
{0} килогерц | ·kk· ·ky· ·mn· ·ru·
{0} килохерц | ·bg· ·mk· ·sr·
{0} кілагерц | ·be·
{0} кілогерц | ·uk·
{0} კილოჰერცი | ·ka·
{0} կիլոհերց | ·hy·
{0} كيلو هرتز | ·ar·
{0} کیلوهرتز | ·fa·
{0} किलोहर्ट्ज़ | ·hi·
{0} किलोहर्ट्झ | ·mr·
{0} কিলোহার্জ | ·bn·
{0} ਕਿਲੋਹਰਟਜ਼ | ·pa·
{0} કિલોહર્ટ્ઝ | ·gu·
{0} கிலோஹெர்ட்ஸ் | ·ta·
{0} కిలోహెర్ట్‌జ్ | ·te·
{0} ಕಿಲೋಹರ್ಟ್ಸ್‌ | ·kn·
{0} കിലോഹെർട്സ് | ·ml·
{0} ᎠᎦᏴᎵᎭᏥ | ·chr·
{0}किलोहर्ज | ·ne·
kilohezi {0} | ·sw·
קילו-הרץ {0} | ·he·
කිලෝහට්ස් {0} | ·si·
long-two | English: ‹{0} kHz›
{0} chile-hertz | ·gd·
{0} chiliheirts | ·ga·
{0} ciloherts | ·cy·
{0} gilohertz | ·br·
{0} kilohertza | ·dsb· ·sl·
{0} kilohertzaj | ·hsb·
{0} קילו-הרץ | ·he·
{0} كيلو هرتز | ·ar·
long-few | English: ‹{0} kHz›
{0} c'hilohertz | ·br·
{0} chiliheirts | ·ga·
{0} cile-hertz | ·gd·
{0} ciloherts | ·cy·
{0} kiloherca | ·bs· ·hr· ·sr_Latn·
{0} kilohercai | ·lt·
{0} kiloherce | ·pl·
{0} kilohertze | ·sk·
{0} kilohertzi | ·ro· ·sl·
{0} kilohertzy | ·cs· ·dsb· ·hsb·
{0} килогерца | ·ru·
{0} килохерца | ·sr·
{0} кілагерцы | ·be·
{0} кілогерци | ·uk·
{0} كيلو هرتز | ·ar·
long-many | English: ‹{0} kHz›
{0} a gilohertzoù | ·br·
{0} ciloherts | ·cy·
{0} gciliheirts | ·ga·
{0} kiloherco | ·lt·
{0} kiloherców | ·pl·
{0} kilohertza | ·sk·
{0} kilohertzu | ·cs·
{0} килогерц | ·ru·
{0} кілагерц | ·be·
{0} кілогерців | ·uk·
{0} קילו-הרץ | ·he·
{0} كيلو هرتز | ·ar·
long-other | English: ‹{0} kilohertz›
{0} cile-hertz | ·gd·
{0} ciliheirts | ·ga·
{0} ciloherts | ·cy·
{0} de kilohertzi | ·ro·
{0} kHz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
{0} kilogers | ·uz·
{0} kilogerts | ·tk·
{0} kiloherc | ·sq·
{0} kiloherca | ·bs· ·hr· ·pl· ·sr_Latn·
{0} kiloherci | ·lv·
{0} kilohercios | ·ast· ·es· ·es_MX· ·es_US·
{0} kilohercų | ·lt·
{0} kilohers | ·az·
{0} kilohertsi | ·et·
{0} kilohertsiä | ·fi·
{0} kilohertz | ·br· ·da· ·en· ·es_419· ·eu· ·fo· ·fr· ·gl· ·hu· ·id· ·it· ·ms· ·nb· ·nl· ·pt· ·sv· ·tr·
{0} Kilohertz | ·lb·
{0} Kilohertz | ·de·
{0} kílóhertz | ·is·
{0} kilohertzev | ·sl·
{0} kilohertzov | ·sk·
{0} kilohertzow | ·dsb· ·hsb·
{0} kilohertzů | ·cs·
{0} na kilohertz | ·fil·
{0} quilohertzs | ·ca·
{0} κιλοχέρτζ | ·el·
{0} килогерц | ·kk· ·ky· ·mn·
{0} килогерца | ·ru·
{0} килохерца | ·bg· ·sr·
{0} килохерци | ·mk·
{0} кілагерца | ·be·
{0} кілогерца | ·uk·
{0} კილოჰერცი | ·ka·
{0} կիլոհերց | ·hy·
{0} קילו-הרץ | ·he·
{0} كيلو هرتز | ·ar·
{0} کیلوهرتز | ·fa· ·mzn·
{0} किलोहर्ट्ज़ | ·hi·
{0} किलोहर्ट्झ | ·mr·
{0} কিলোহার্জ | ·bn·
{0} ਕਿਲੋਹਰਟਜ਼ | ·pa·
{0} કિલોહર્ટ્ઝ | ·gu·
{0} கிலோஹெர்ட்ஸ் | ·ta·
{0} కిలోహెర్ట్‌జ్ | ·te·
{0} ಕಿಲೋಹರ್ಟ್ಸ್‌ | ·kn·
{0} കിലോഹെർട്സ് | ·ml·
{0} กิโลเฮิรตซ์ | ·th·
{0} ကီလိုဟတ်ဇ် | ·my·
{0} គីឡូហឺត | ·km·
{0} ᎠᎦᏴᎵᎭᏥ | ·chr·
{0} キロヘルツ | ·ja·
{0} 千赫 | ·yue· ·zh_Hant·
{0}किलोहर्ज | ·ne·
{0}킬로헤르츠 | ·ko·
{0}千赫 | ·zh·
kilohēti ʻe {0} | ·to·
kilohezi {0} | ·sw·
කිලෝහට්ස් {0} | ·si·
short-displayName | English: ‹kHz›
kGs | ·tk· ·uz·
kHz | ·all·others·
kilohezi | ·sw·
κιλοχέρτζ | ·el·
кГц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
კჰც. | ·ka·
կՀց | ·hy·
ك هرتز | ·ar·
ک.هرتز | ·fa·
کیلوهرتز | ·mzn·
கி.ஹெஸ். | ·ta·
కి.హె | ·te·
ಕಿ.ಹ | ·kn·
കി.ഹെ. | ·ml·
කිහස් | ·si·
千赫 | ·yue· ·zh· ·zh_Hant·
short-zero | English: ‹{0} kHz›
{0} kHz | ·cy· ·lv·
{0} ك هرتز | ·ar·
short-one | English: ‹{0} kHz›
{0} kGs | ·tk· ·uz·
{0} kHz | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tr· ·ur· ·zu·
{0} кГц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} კჰც. | ·ka·
{0} կՀց | ·hy·
{0} ك هرتز | ·ar·
{0} ک.هرتز | ·fa·
{0} கி.ஹெஸ். | ·ta·
{0} కి.హె | ·te·
{0} ಕಿ.ಹ | ·kn·
{0} കി.ഹെ. | ·ml·
kilohezi {0} | ·sw·
කිහස් {0} | ·si·
short-two | English: ‹{0} kHz›
{0} kHz | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} ك هرتز | ·ar·
short-few | English: ‹{0} kHz›
{0} kHz | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} кГц | ·be· ·ru· ·uk·
{0} ك هرتز | ·ar·
short-many | English: ‹{0} kHz›
{0} kHz | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} кГц | ·be· ·ru· ·uk·
{0} ك هرتز | ·ar·
short-other | English: ‹{0} kHz›
{0} kGs | ·tk· ·uz·
{0} kHz | ·all·others·
{0} кГц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} კჰც. | ·ka·
{0} կՀց | ·hy·
{0} ك هرتز | ·ar·
{0} ک.هرتز | ·fa·
{0} கி.ஹெஸ். | ·ta·
{0} కి.హె | ·te·
{0} ಕಿ.ಹ | ·kn·
{0} കി.ഹെ. | ·ml·
{0} 千赫 | ·yue· ·zh_Hant·
{0}kHz | ·ko·
{0}千赫 | ·zh·
kHz ʻe {0} | ·to·
kilohezi {0} | ·sw·
කිහස් {0} | ·si·
narrow-displayName | English: ‹kHz›
kHz | ·ast· ·cs· ·cy· ·en· ·fi· ·ga· ·gd· ·sv· ·to·
ک.هرتز | ·fa·
narrow-zero | English: ‹{0} kHz›
{0}kHz | ·cy·
narrow-one | English: ‹{0}kHz›
{0} kHz | ·cs· ·de· ·hr· ·nl· ·tr·
{0} ک.هرتز | ·fa·
{0}kHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} kHz›
{0}kHz | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} kHz›
{0} kHz | ·cs· ·hr·
{0}kHz | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} kHz›
{0} kHz | ·cs·
{0}kHz | ·cy· ·ga·
narrow-other | English: ‹{0}kHz›
{0} kHz | ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0} ک.هرتز | ·fa·
{0}kHz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·
hertz
long-displayName | English: ‹hertz›
gers | ·uz·
gerts | ·tk·
heirts | ·ga·
herc | ·sq·
hercai | ·lt·
herce | ·pl·
herci | ·bs· ·hr· ·lv· ·sr_Latn·
hercios | ·ast· ·es· ·es_MX· ·es_US·
hers | ·az·
herts | ·cy·
hertsid | ·et·
hertsit | ·fi·
hertz | ·ca· ·da· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·gd· ·gl· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·pt· ·ro· ·sl· ·sv· ·tr·
Hertz | ·de· ·lb·
hertze | ·sk·
hertzoù | ·br·
hertzy | ·cs· ·dsb· ·hsb·
hēti | ·to·
hezi | ·sw·
Hz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
χερτζ | ·el·
герц | ·kk· ·ky· ·mn· ·sah·
герци | ·uk·
герцы | ·be· ·ru·
херц | ·mk·
херци | ·sr·
херцове | ·bg·
ჰერცი | ·ka·
հերցեր | ·hy·
הרץ | ·he·
هرتز | ·ar· ·fa· ·mzn·
हर्ज | ·ne·
हर्ट्ज़ | ·hi·
हर्ट्झ | ·mr·
হার্জ | ·bn·
ਹਰਟਜ਼ | ·pa·
હર્ટ્ઝ | ·gu·
ஹெர்ட்ஸ் | ·ta·
హెర్ట్‌జ్ | ·te·
ಹರ್ಟ್ಸ್‌ | ·kn·
ഹെർട്സ് | ·ml·
හට්ස් | ·si·
เฮิรตซ์ | ·th·
ဟတ်ဇ် | ·my·
ហឺត | ·km·
ᎭᏥ | ·chr·
헤르츠 | ·ko·
ヘルツ | ·ja·
赫兹 | ·zh·
赫茲 | ·yue· ·zh_Hant·
long-zero | English: ‹{0} Hz›
{0} herci | ·lv·
{0} herts | ·cy·
{0} هرتز | ·ar·
long-one | English: ‹{0} hertz›
{0} gers | ·uz·
{0} gerts | ·tk·
{0} heirts | ·ga·
{0} herc | ·bs· ·hr· ·pl· ·sq· ·sr_Latn·
{0} hercas | ·lt·
{0} hercio | ·es· ·es_MX· ·es_US·
{0} herciu | ·ast·
{0} hercs | ·lv·
{0} hers | ·az·
{0} herts | ·cy· ·et·
{0} hertsi | ·fi·
{0} hertz | ·br· ·ca· ·cs· ·da· ·dsb· ·en· ·es_419· ·eu· ·fil· ·fo· ·fr· ·gd· ·gl· ·hsb· ·hu· ·is· ·it· ·nb· ·nl· ·pt· ·ro· ·sk· ·sl· ·sv· ·tr·
{0} Hertz | ·lb·
{0} Hertz | ·de·
{0} Hz | ·af· ·am· ·ur· ·zu·
{0} χερτζ | ·el·
{0} герц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} херц | ·bg· ·mk· ·sr·
{0} ჰერცი | ·ka·
{0} հերց | ·hy·
{0} هرتز | ·ar· ·fa·
{0} हर्ज | ·ne·
{0} हर्ट्ज़ | ·hi·
{0} हर्ट्झ | ·mr·
{0} হার্জ | ·bn·
{0} ਹਰਟਜ਼ | ·pa·
{0} હર્ટ્ઝ | ·gu·
{0} ஹெர்ட்ஸ் | ·ta·
{0} హెర్ట్‌జ్ | ·te·
{0} ಹರ್ಟ್ಸ್‌ | ·kn·
{0} ഹെർട്സ് | ·ml·
{0} ᎭᏥ | ·chr·
hezi {0} | ·sw·
הרץ {0} | ·he·
හට්ස් {0} | ·si·
long-two | English: ‹{0} Hz›
{0} heirts | ·ga·
{0} herts | ·cy·
{0} hertz | ·br· ·gd·
{0} hertza | ·dsb· ·sl·
{0} hertzaj | ·hsb·
{0} הרץ | ·he·
{0} هرتز | ·ar·
long-few | English: ‹{0} Hz›
{0} heirts | ·ga·
{0} herca | ·bs· ·hr· ·sr_Latn·
{0} hercai | ·lt·
{0} herce | ·pl·
{0} herts | ·cy·
{0} hertz | ·br· ·gd·
{0} hertze | ·sk·
{0} hertzi | ·ro· ·sl·
{0} hertzy | ·cs· ·dsb· ·hsb·
{0} герца | ·ru·
{0} герци | ·uk·
{0} герцы | ·be·
{0} херца | ·sr·
{0} هرتز | ·ar·
long-many | English: ‹{0} Hz›
{0} a hertzoù | ·br·
{0} heirts | ·ga·
{0} herco | ·lt·
{0} herców | ·pl·
{0} herts | ·cy·
{0} hertza | ·sk·
{0} hertzu | ·cs·
{0} герц | ·be· ·ru·
{0} герців | ·uk·
{0} הרץ | ·he·
{0} هرتز | ·ar·
long-other | English: ‹{0} hertz›
{0} de hertzi | ·ro·
{0} gers | ·uz·
{0} gerts | ·tk·
{0} heirts | ·ga·
{0} herc | ·sq·
{0} herca | ·bs· ·hr· ·pl· ·sr_Latn·
{0} herci | ·lv·
{0} hercios | ·ast· ·es· ·es_MX· ·es_US·
{0} hercų | ·lt·
{0} hers | ·az·
{0} herts | ·cy·
{0} hertsi | ·et·
{0} hertsiä | ·fi·
{0} hertz | ·br· ·da· ·en· ·es_419· ·eu· ·fo· ·fr· ·gd· ·gl· ·hu· ·id· ·is· ·it· ·ms· ·nb· ·nl· ·pt· ·sv· ·tr·
{0} Hertz | ·lb·
{0} Hertz | ·de·
{0} hertzev | ·sl·
{0} hertzov | ·sk·
{0} hertzow | ·dsb· ·hsb·
{0} hertzs | ·ca·
{0} hertzů | ·cs·
{0} Hz | ·af· ·am· ·lo· ·ur· ·vi· ·zu·
{0} na hertz | ·fil·
{0} χερτζ | ·el·
{0} герц | ·kk· ·ky· ·mn· ·sah·
{0} герца | ·be· ·ru· ·uk·
{0} херца | ·bg· ·sr·
{0} херци | ·mk·
{0} ჰერცი | ·ka·
{0} հերց | ·hy·
{0} הרץ | ·he·
{0} هرتز | ·ar· ·fa· ·mzn·
{0} हर्ज | ·ne·
{0} हर्ट्ज़ | ·hi·
{0} हर्ट्झ | ·mr·
{0} হার্জ | ·bn·
{0} ਹਰਟਜ਼ | ·pa·
{0} હર્ટ્ઝ | ·gu·
{0} ஹெர்ட்ஸ் | ·ta·
{0} హెర్ట్‌జ్ | ·te·
{0} ಹರ್ಟ್ಸ್‌ | ·kn·
{0} ഹെർട്സ് | ·ml·
{0} เฮิรตซ์ | ·th·
{0} ဟတ်ဇ် | ·my·
{0} ហឺត | ·km·
{0} ᎭᏥ | ·chr·
{0} ヘルツ | ·ja·
{0} 赫茲 | ·yue· ·zh_Hant·
{0}헤르츠 | ·ko·
{0}赫兹 | ·zh·
hēti ʻe {0} | ·to·
hezi {0} | ·sw·
හට්ස් {0} | ·si·
short-displayName | English: ‹Hz›
Gs | ·tk· ·uz·
hezi | ·sw·
Hz | ·all·others·
χερτζ | ·el·
Гц | ·be· ·kk· ·ky· ·mn· ·ru· ·sah· ·uk·
ჰც. | ·ka·
Հց | ·hy·
هرتز | ·ar· ·fa· ·mzn·
હર્ટ્ઝ | ·gu·
ஹெஸ். | ·ta·
హెర్ట్‌జ్ | ·te·
ಹರ್ಟ್ಸ್‌ | ·kn·
ഹെ. | ·ml·
හස් | ·si·
赫兹 | ·zh·
赫茲 | ·yue· ·zh_Hant·
short-zero | English: ‹{0} Hz›
{0} Hz | ·cy· ·lv·
{0} هرتز | ·ar·
short-one | English: ‹{0} Hz›
{0} Gs | ·tk· ·uz·
{0} Hz | ·af· ·am· ·ast· ·az· ·bg· ·bn· ·br· ·bs· ·ca· ·chr· ·cs· ·cy· ·da· ·de· ·dsb· ·el· ·en· ·es· ·et· ·eu· ·fi· ·fil· ·fo· ·fr· ·ga· ·gd· ·gl· ·gu· ·he· ·hi· ·hr· ·hsb· ·hu· ·is· ·it· ·lb· ·lt· ·lv· ·mk· ·mr· ·nb· ·ne· ·nl· ·pa· ·pl· ·pt· ·ro· ·sk· ·sl· ·sq· ·sr· ·sr_Latn· ·sv· ·tr· ·ur· ·zu·
{0} Гц | ·be· ·kk· ·ky· ·mn· ·ru· ·uk·
{0} ჰც. | ·ka·
{0} Հց | ·hy·
{0} هرتز | ·ar· ·fa·
{0} ஹெஸ். | ·ta·
{0} హెర్ట్‌జ్ | ·te·
{0} ಹರ್ಟ್ಸ್‌ | ·kn·
{0} ഹെ. | ·ml·
hezi {0} | ·sw·
හස් {0} | ·si·
short-two | English: ‹{0} Hz›
{0} Hz | ·br· ·cy· ·dsb· ·ga· ·gd· ·he· ·hsb· ·sl·
{0} هرتز | ·ar·
short-few | English: ‹{0} Hz›
{0} Hz | ·br· ·bs· ·cs· ·cy· ·dsb· ·ga· ·gd· ·hr· ·hsb· ·lt· ·pl· ·ro· ·sk· ·sl· ·sr· ·sr_Latn·
{0} Гц | ·be· ·ru· ·uk·
{0} هرتز | ·ar·
short-many | English: ‹{0} Hz›
{0} Hz | ·br· ·cs· ·cy· ·ga· ·he· ·lt· ·pl· ·sk·
{0} Гц | ·be· ·ru· ·uk·
{0} هرتز | ·ar·
short-other | English: ‹{0} Hz›
{0} Gs | ·tk· ·uz·
{0} Hz | ·all·others·
{0} Гц | ·be· ·kk· ·ky· ·mn· ·ru· ·sah· ·uk·
{0} ჰც. | ·ka·
{0} Հց | ·hy·
{0} هرتز | ·ar· ·fa·
{0} ஹெஸ். | ·ta·
{0} హెర్ట్‌జ్ | ·te·
{0} ಹರ್ಟ್ಸ್‌ | ·kn·
{0} ഹെ. | ·ml·
{0} 赫茲 | ·yue· ·zh_Hant·
{0}Hz | ·ko·
{0}赫 | ·zh·
hezi {0} | ·sw·
Hz ʻe {0} | ·to·
හස් {0} | ·si·
narrow-displayName | English: ‹Hz›
Hz | ·ast· ·cs· ·cy· ·en· ·fi· ·ga· ·gd· ·sv· ·to·
narrow-zero | English: ‹{0} Hz›
{0}Hz | ·cy·
narrow-one | English: ‹{0}Hz›
{0} Hz | ·ca· ·cs· ·de· ·hr· ·nl· ·tr·
{0}Hz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·pa· ·sv·
narrow-two | English: ‹{0} Hz›
{0}Hz | ·cy· ·ga· ·gd·
narrow-few | English: ‹{0} Hz›
{0} Hz | ·cs· ·hr·
{0}Hz | ·cy· ·ga· ·gd·
narrow-many | English: ‹{0} Hz›
{0} Hz | ·cs·
{0}Hz | ·cy· ·ga·
narrow-other | English: ‹{0}Hz›
{0} Hz | ·ca· ·cs· ·de· ·hr· ·nl· ·to· ·tr·
{0}Hz | ·ast· ·cy· ·en· ·fi· ·ga· ·gd· ·ja· ·pa· ·sv· ·yue· ·zh_Hant·