Go to the first, previous, next, last section, table of contents.

# Assembler Directives

All assembler directives have names that begin with a period (``.'`). The rest of the name is letters, usually in lower case.

This chapter discusses directives that are available regardless of the target machine configuration for the GNU assembler. Some machine configurations provide additional directives. See section Machine Dependent Features.

- Abort: `.abort`
- ABORT: `.ABORT`
- Align: `.align abs-expr` , abs-expr
- App-File: `.app-file string`
- Ascii: `.ascii "string`"...
- Asciz: `.asciz "string`"...
- Balign: `.balign abs-expr` , abs-expr
- Byte: `.byte expressions`
- Comm: `.comm symbol` , length
- Data: `.data subsection`
- Def: `.def name`
- Desc: `.desc symbol`, abs-expression
- Dim: `.dim`
- Double: `.double flonums`
- Eject: `.eject`
- Else: `.else`
- Endef: `.endef`
- Endif: `.endif`
- Equ: `.equ symbol`, expression
- Equiv: `.equiv symbol`, expression
- Err: `.err`
- Extern: `.extern`
- File: `.file string`
- Fill: `.fill repeat` , size , value
- Float: `.float flonums`
- Global: `.global symbol`, `.globl symbol`
- hword: `.hword expressions`
- Ident: `.ident`
- If: `.if absolute expression`
- Include: `.include "file`"
- Int: `.int expressions`
- Irp: `.irp symbol`,values...
- Irpc: `.irpc symbol`,values...
- Lcomm: `.lcomm symbol` , length
- Lflags: `.lflags`
- Line: `.line line-number`
- Ln: `.ln line-number`
- Linkonce: `.linkonce [type`]
- List: `.list`
- Long: `.long expressions`
- Macro: `.macro name` args...
- MRI: `.mri val`
- Nolist: `.nolist`
- Octa: `.octa bignums`
- Org: `.org new-lc` , fill
- P2align: `.p2align abs-expr` , abs-expr
- Psize: `.psize lines`, columns
- Quad: `.quad bignums`
- Rept: `.rept count`
- Sbttl: `.sbttl "subheading`"
- Scl: `.scl class`
- Section: `.section name`, subsection
- Set: `.set symbol`, expression
- Short: `.short expressions`
- Single: `.single flonums`
- Size: `.size`
- Skip: `.skip size` , fill
- Space: `.space size` , fill
- Stab: `.stabd, .stabn, .stabs`
- String: `.string "str`"
- Symver: `.symver name`,name2@nodename
- Tag: `.tag structname`
- Text: `.text subsection`
- Title: `.title "heading`"
- Type: `.type int`
- Val: `.val addr`
- Word: `.word expressions`
- Deprecated: Deprecated Directives

## `.abort`

This directive stops the assembly immediately. It is for compatibility with other assemblers. The original idea was that the assembly language source would be piped into the assembler. If the sender of the source quit, it could use this directive tells `as` to quit also. One day `.abort` will not be supported.

## `.ABORT`

When producing COFF output, `as` accepts this directive as a synonym for ``.abort'`.

When producing `b.out` output, `as` accepts this directive, but ignores it.

## `.align abs-expr, abs-expr, abs-expr`

Pad the location counter (in the current subsection) to a particular storage boundary. The first expression (which must be absolute) is the alignment required, as described below.

The second expression (also absolute) gives the fill value to be stored in the padding bytes. It (and the comma) may be omitted. If it is omitted, the padding bytes are normally zero. However, on some systems, if the section is marked as containing code and the fill value is omitted, the space is filled with no-op instructions.

The third expression is also absolute, and is also optional. If it is present, it is the maximum number of bytes that should be skipped by this alignment directive. If doing the alignment would require skipping more bytes than the specified maximum, then the alignment is not done at all. You can omit the fill value (the second argument) entirely by simply using two commas after the required alignment; this can be useful if you want the alignment to be filled with no-op instructions when appropriate.

The way the required alignment is specified varies from system to system. For the a29k, hppa, m68k, m88k, w65, sparc, and Hitachi SH, and i386 using ELF format, the first expression is the alignment request in bytes. For example ``.align 8'` advances the location counter until it is a multiple of 8. If the location counter is already a multiple of 8, no change is needed.

For other systems, including the i386 using a.out format, it is the number of low-order zero bits the location counter must have after advancement. For example ``.align 3'` advances the location counter until it a multiple of 8. If the location counter is already a multiple of 8, no change is needed.

This inconsistency is due to the different behaviors of the various native assemblers for these systems which GAS must emulate. GAS also provides `.balign` and `.p2align` directives, described later, which have a consistent behavior across all architectures (but are specific to GAS).

## `.app-file string`

`.app-file` (which may also be spelled ``.file'`) tells `as` that we are about to start a new logical file. string is the new file name. In general, the filename is recognized whether or not it is surrounded by quotes ``"'`; but if you wish to specify an empty file name is permitted, you must give the quotes--`""`. This statement may go away in future: it is only recognized to be compatible with old `as` programs.

## `.ascii "string"`...

`.ascii` expects zero or more string literals (see section Strings) separated by commas. It assembles each string (with no automatic trailing zero byte) into consecutive addresses.

## `.asciz "string"`...

`.asciz` is just like `.ascii`, but each string is followed by a zero byte. The "z" in ``.asciz'` stands for "zero".

## `.balign[wl] abs-expr, abs-expr, abs-expr`

Pad the location counter (in the current subsection) to a particular storage boundary. The first expression (which must be absolute) is the alignment request in bytes. For example ``.balign 8'` advances the location counter until it is a multiple of 8. If the location counter is already a multiple of 8, no change is needed.

The second expression (also absolute) gives the fill value to be stored in the padding bytes. It (and the comma) may be omitted. If it is omitted, the padding bytes are normally zero. However, on some systems, if the section is marked as containing code and the fill value is omitted, the space is filled with no-op instructions.

The third expression is also absolute, and is also optional. If it is present, it is the maximum number of bytes that should be skipped by this alignment directive. If doing the alignment would require skipping more bytes than the specified maximum, then the alignment is not done at all. You can omit the fill value (the second argument) entirely by simply using two commas after the required alignment; this can be useful if you want the alignment to be filled with no-op instructions when appropriate.

The `.balignw` and `.balignl` directives are variants of the `.balign` directive. The `.balignw` directive treats the fill pattern as a two byte word value. The `.balignl` directives treats the fill pattern as a four byte longword value. For example, `.balignw 4,0x368d` will align to a multiple of 4. If it skips two bytes, they will be filled in with the value 0x368d (the exact placement of the bytes depends upon the endianness of the processor). If it skips 1 or 3 bytes, the fill value is undefined.

## `.byte expressions`

`.byte` expects zero or more expressions, separated by commas. Each expression is assembled into the next byte.

## `.comm symbol , length`

`.comm` declares a common symbol named symbol. When linking, a common symbol in one object file may be merged with a defined or common symbol of the same name in another object file. If `ld` does not see a definition for the symbol--just one or more common symbols--then it will allocate length bytes of uninitialized memory. length must be an absolute expression. If `ld` sees multiple common symbols with the same name, and they do not all have the same size, it will allocate space using the largest size.

When using ELF, the `.comm` directive takes an optional third argument. This is the desired alignment of the symbol, specified as a byte boundary (for example, an alignment of 16 means that the least significant 4 bits of the address should be zero). The alignment must be an absolute expression, and it must be a power of two. If `ld` allocates uninitialized memory for the common symbol, it will use the alignment when placing the symbol. If no alignment is specified, `as` will set the alignment to the largest power of two less than or equal to the size of the symbol, up to a maximum of 16.

The syntax for `.comm` differs slightly on the HPPA. The syntax is ``symbol .comm, length'`; symbol is optional.

## `.data subsection`

`.data` tells `as` to assemble the following statements onto the end of the data subsection numbered subsection (which is an absolute expression). If subsection is omitted, it defaults to zero.

## `.def name`

Begin defining debugging information for a symbol name; the definition extends until the `.endef` directive is encountered.

This directive is only observed when `as` is configured for COFF format output; when producing `b.out`, ``.def'` is recognized, but ignored.

## `.desc symbol, abs-expression`

This directive sets the descriptor of the symbol (see section Symbol Attributes) to the low 16 bits of an absolute expression.

The ``.desc'` directive is not available when `as` is configured for COFF output; it is only for `a.out` or `b.out` object format. For the sake of compatibility, `as` accepts it, but produces no output, when configured for COFF.

## `.dim`

This directive is generated by compilers to include auxiliary debugging information in the symbol table. It is only permitted inside `.def`/`.endef` pairs.

``.dim'` is only meaningful when generating COFF format output; when `as` is generating `b.out`, it accepts this directive but ignores it.

## `.double flonums`

`.double` expects zero or more flonums, separated by commas. It assembles floating point numbers. The exact kind of floating point numbers emitted depends on how `as` is configured. See section Machine Dependent Features.

## `.eject`

Force a page break at this point, when generating assembly listings.

## `.else`

`.else` is part of the `as` support for conditional assembly; see section `.if absolute expression`. It marks the beginning of a section of code to be assembled if the condition for the preceding `.if` was false.

## `.endef`

This directive flags the end of a symbol definition begun with `.def`.

``.endef'` is only meaningful when generating COFF format output; if `as` is configured to generate `b.out`, it accepts this directive but ignores it.

## `.endif`

`.endif` is part of the `as` support for conditional assembly; it marks the end of a block of code that is only assembled conditionally. See section `.if absolute expression`.

## `.equ symbol, expression`

This directive sets the value of symbol to expression. It is synonymous with ``.set'`; see section `.set symbol`, expression.

The syntax for `equ` on the HPPA is ``symbol .equ expression'`.

## `.equiv symbol, expression`

The `.equiv` directive is like `.equ` and `.set`, except that the assembler will signal an error if symbol is already defined.

Except for the contents of the error message, this is roughly equivalent to

    .ifdef SYM
    .err
    .endif
    .equ SYM,VAL

## `.err`

If `as` assembles a `.err` directive, it will print an error message and, unless the `-Z` option was used, it will not generate an object file. This can be used to signal error an conditionally compiled code.

## `.extern`

`.extern` is accepted in the source program--for compatibility with other assemblers--but it is ignored. `as` treats all undefined symbols as external.

## `.file string`

`.file` (which may also be spelled ``.app-file'`) tells `as` that we are about to start a new logical file. string is the new file name. In general, the filename is recognized whether or not it is surrounded by quotes ``"'`; but if you wish to specify an empty file name, you must give the quotes--`""`. This statement may go away in future: it is only recognized to be compatible with old `as` programs. In some configurations of `as`, `.file` has already been removed to avoid conflicts with other assemblers. See section Machine Dependent Features.

## `.fill repeat , size , value`

result, size and value are absolute expressions. This emits repeat copies of size bytes. Repeat may be zero or more. Size may be zero or more, but if it is more than 8, then it is deemed to have the value 8, compatible with other people's assemblers. The contents of each repeat bytes is taken from an 8-byte number. The highest order 4 bytes are zero. The lowest order 4 bytes are value rendered in the byte-order of an integer on the computer `as` is assembling for. Each size bytes in a repetition is taken from the lowest order size bytes of this number. Again, this bizarre behavior is compatible with other people's assemblers.

size and value are optional. If the second comma and value are absent, value is assumed zero. If the first comma and following tokens are absent, size is assumed to be 1.

## `.float flonums`

This directive assembles zero or more flonums, separated by commas. It has the same effect as `.single`. The exact kind of floating point numbers emitted depends on how `as` is configured. See section Machine Dependent Features.

## `.global symbol`, `.globl symbol`

`.global` makes the symbol visible to `ld`. If you define symbol in your partial program, its value is made available to other partial programs that are linked with it. Otherwise, symbol takes its attributes from a symbol of the same name from another file linked into the same program.

Both spellings (``.globl'` and ``.global'`) are accepted, for compatibility with other assemblers.

On the HPPA, `.global` is not always enough to make it accessible to other partial programs. You may need the HPPA-only `.EXPORT` directive as well. See section HPPA Assembler Directives.

## `.hword expressions`

This expects zero or more expressions, and emits a 16 bit number for each.

This directive is a synonym for ``.short'`; depending on the target architecture, it may also be a synonym for ``.word'`.

## `.ident`

This directive is used by some assemblers to place tags in object files. `as` simply accepts the directive for source-file compatibility with such assemblers, but does not actually emit anything for it.

## `.if absolute expression`

`.if` marks the beginning of a section of code which is only considered part of the source program being assembled if the argument (which must be an absolute expression) is non-zero. The end of the conditional section of code must be marked by `.endif` (see section `.endif`); optionally, you may include code for the alternative condition, flagged by `.else` (see section `.else`).

The following variants of `.if` are also supported:

`.ifdef symbol`
  Assembles the following section of code if the specified symbol has been defined.
`.ifndef symbol`
`.ifnotdef symbol`
  Assembles the following section of code if the specified symbol has not been defined. Both spelling variants are equivalent.

## `.include "file"`

This directive provides a way to include supporting files at specified points in your source program. The code from file is assembled as if it followed the point of the `.include`; when the end of the included file is reached, assembly of the original file continues. You can control the search paths used with the ``-I'` command-line option (see section Command-Line Options). Quotation marks are required around file.

## `.int expressions`

Expect zero or more expressions, of any section, separated by commas. For each expression, emit a number that, at run time, is the value of that expression. The byte order and bit size of the number depends on what kind of target the assembly is for.

## `.irp symbol,values`...

Evaluate a sequence of statements assigning different values to symbol. The sequence of statements starts at the `.irp` directive, and is terminated by an `.endr` directive. For each value, symbol is set to value, and the sequence of statements is assembled. If no value is listed, the sequence of statements is assembled once, with symbol set to the null string. To refer to symbol within the sequence of statements, use \symbol.

For example, assembling

            .irp    param,1,2,3
            move    d\param,sp@-
            .endr

is equivalent to assembling

            move    d1,sp@-
            move    d2,sp@-
            move    d3,sp@-

## `.irpc symbol,values`...

Evaluate a sequence of statements assigning different values to symbol. The sequence of statements starts at the `.irpc` directive, and is terminated by an `.endr` directive. For each character in value, symbol is set to the character, and the sequence of statements is assembled. If no value is listed, the sequence of statements is assembled once, with symbol set to the null string. To refer to symbol within the sequence of statements, use \symbol.

For example, assembling

            .irpc    param,123
            move    d\param,sp@-
            .endr

is equivalent to assembling

            move    d1,sp@-
            move    d2,sp@-
            move    d3,sp@-

## `.lcomm symbol , length`

Reserve length (an absolute expression) bytes for a local common denoted by symbol. The section and value of symbol are those of the new local common. The addresses are allocated in the bss section, so that at run-time the bytes start off zeroed. Symbol is not declared global (see section `.global symbol`, `.globl symbol`), so is normally not visible to `ld`.

Some targets permit a third argument to be used with `.lcomm`. This argument specifies the desired alignment of the symbol in the bss section.

The syntax for `.lcomm` differs slightly on the HPPA. The syntax is ``symbol .lcomm, length'`; symbol is optional.

## `.lflags`

`as` accepts this directive, for compatibility with other assemblers, but ignores it.

## `.line line-number`

Change the logical line number. line-number must be an absolute expression. The next line has that logical line number. Therefore any other statements on the current line (after a statement separator character) are reported as on logical line number line-number - 1. One day `as` will no longer support this directive: it is recognized only for compatibility with existing assembler programs.

Warning: In the AMD29K configuration of as, this command is not available; use the synonym `.ln` in that context.

Even though this is a directive associated with the `a.out` or `b.out` object-code formats, `as` still recognizes it when producing COFF output, and treats ``.line'` as though it were the COFF ``.ln'` if it is found outside a `.def`/`.endef` pair.

Inside a `.def`, ``.line'` is, instead, one of the directives used by compilers to generate auxiliary symbol information for debugging.

## `.linkonce [type]`

Mark the current section so that the linker only includes a single copy of it. This may be used to include the same section in several different object files, but ensure that the linker will only include it once in the final output file. The `.linkonce` pseudo-op must be used for each instance of the section. Duplicate sections are detected based on the section name, so it should be unique.

This directive is only supported by a few object file formats; as of this writing, the only object file format which supports it is the Portable Executable format used on Windows NT.

The type argument is optional. If specified, it must be one of the following strings. For example:

    .linkonce same_size

Not all types may be supported on all object file formats.

`discard`
  Silently discard duplicate sections. This is the default.
`one_only`
  Warn if there are duplicate sections, but still keep only one copy.
`same_size`
  Warn if any of the duplicates have different sizes.
`same_contents`
  Warn if any of the duplicates do not have exactly the same contents.

## `.ln line-number`

``.ln'` is a synonym for ``.line'`.

## `.mri val`

If val is non-zero, this tells `as` to enter MRI mode. If val is zero, this tells `as` to exit MRI mode. This change affects code assembled until the next `.mri` directive, or until the end of the file. See section Assemble in MRI Compatibility Mode: `-M`.

## `.list`

Control (in conjunction with the `.nolist` directive) whether or not assembly listings are generated. These two directives maintain an internal counter (which is zero initially). `.list` increments the counter, and `.nolist` decrements it. Assembly listings are generated whenever the counter is greater than zero.

By default, listings are disabled. When you enable them (with the ``-a'` command line option; see section Command-Line Options), the initial value of the listing counter is one.

## `.long expressions`

`.long` is the same as ``.int'`, see section `.int expressions`.

## `.macro`

The commands `.macro` and `.endm` allow you to define macros that generate assembly output. For example, this definition specifies a macro `sum` that puts a sequence of numbers into memory:

            .macro  sum from=0, to=5
            .long   \from
            .if     \to-\from
            sum     "(\from+1)",\to
            .endif
            .endm

With that definition, ``SUM 0,5'` is equivalent to this assembly input:

            .long   0
            .long   1
            .long   2
            .long   3
            .long   4
            .long   5

`.macro macname`
`.macro macname macargs ...`
  Begin the definition of a macro called macname. If your macro definition requires arguments, specify their names after the macro name, separated by commas or spaces. You can supply a default value for any macro argument by following the name with ``=deflt'`. For example, these are all valid `.macro` statements:
  `.macro comm`
    Begin the definition of a macro called `comm`, which takes no arguments.
  `.macro plus1 p, p1`
  `.macro plus1 p p1`
    Either statement begins the definition of a macro called `plus1`, which takes two arguments; within the macro definition, write ``\p'` or ``\p1'` to evaluate the arguments.
  `.macro reserve_str p1=0 p2`
    Begin the definition of a macro called `reserve_str`, with two arguments. The first argument has a default value, but not the second. After the definition is complete, you can call the macro either as ``reserve_str a,b'` (with ``\p1'` evaluating to a and ``\p2'` evaluating to b), or as ``reserve_str ,b'` (with ``\p1'` evaluating as the default, in this case ``0'`, and ``\p2'` evaluating to b).
  When you call a macro, you can specify the argument values either by position, or by keyword. For example, ``sum 9,17'` is equivalent to ``sum to=17, from=9'`.
`.endm`
  Mark the end of a macro definition.
`.exitm`
  Exit early from the current macro definition.
`\@`
  `as` maintains a counter of how many macros it has executed in this pseudo-variable; you can copy that number to your output with ``\@'`, but only within a macro definition.

## `.nolist`

Control (in conjunction with the `.list` directive) whether or not assembly listings are generated. These two directives maintain an internal counter (which is zero initially). `.list` increments the counter, and `.nolist` decrements it. Assembly listings are generated whenever the counter is greater than zero.

## `.octa bignums`

This directive expects zero or more bignums, separated by commas. For each bignum, it emits a 16-byte integer.

The term "octa" comes from contexts in which a "word" is two bytes; hence octa-word for 16 bytes.

## `.org new-lc , fill`

Advance the location counter of the current section to new-lc. new-lc is either an absolute expression or an expression with the same section as the current subsection. That is, you can't use `.org` to cross sections: if new-lc has the wrong section, the `.org` directive is ignored. To be compatible with former assemblers, if the section of new-lc is absolute, `as` issues a warning, then pretends the section of new-lc is the same as the current subsection.

`.org` may only increase the location counter, or leave it unchanged; you cannot use `.org` to move the location counter backwards.

Because `as` tries to assemble programs in one pass, new-lc may not be undefined. If you really detest this restriction we eagerly await a chance to share your improved assembler.

Beware that the origin is relative to the start of the section, not to the start of the subsection. This is compatible with other people's assemblers.

When the location counter (of the current subsection) is advanced, the intervening bytes are filled with fill which should be an absolute expression. If the comma and fill are omitted, fill defaults to zero.

## `.p2align[wl] abs-expr, abs-expr, abs-expr`

Pad the location counter (in the current subsection) to a particular storage boundary. The first expression (which must be absolute) is the number of low-order zero bits the location counter must have after advancement. For example ``.p2align 3'` advances the location counter until it a multiple of 8. If the location counter is already a multiple of 8, no change is needed.

The second expression (also absolute) gives the fill value to be stored in the padding bytes. It (and the comma) may be omitted. If it is omitted, the padding bytes are normally zero. However, on some systems, if the section is marked as containing code and the fill value is omitted, the space is filled with no-op instructions.

The third expression is also absolute, and is also optional. If it is present, it is the maximum number of bytes that should be skipped by this alignment directive. If doing the alignment would require skipping more bytes than the specified maximum, then the alignment is not done at all. You can omit the fill value (the second argument) entirely by simply using two commas after the required alignment; this can be useful if you want the alignment to be filled with no-op instructions when appropriate.

The `.p2alignw` and `.p2alignl` directives are variants of the `.p2align` directive. The `.p2alignw` directive treats the fill pattern as a two byte word value. The `.p2alignl` directives treats the fill pattern as a four byte longword value. For example, `.p2alignw 2,0x368d` will align to a multiple of 4. If it skips two bytes, they will be filled in with the value 0x368d (the exact placement of the bytes depends upon the endianness of the processor). If it skips 1 or 3 bytes, the fill value is undefined.

## `.psize lines , columns`

Use this directive to declare the number of lines--and, optionally, the number of columns--to use for each page, when generating listings.

If you do not use `.psize`, listings use a default line-count of 60. You may omit the comma and columns specification; the default width is 200 columns.

`as` generates formfeeds whenever the specified number of lines is exceeded (or whenever you explicitly request one, using `.eject`).

If you specify lines as `0`, no formfeeds are generated save those explicitly specified with `.eject`.

## `.quad bignums`

`.quad` expects zero or more bignums, separated by commas. For each bignum, it emits an 8-byte integer. If the bignum won't fit in 8 bytes, it prints a warning message; and just takes the lowest order 8 bytes of the bignum.

The term "quad" comes from contexts in which a "word" is two bytes; hence quad-word for 8 bytes.

## `.rept count`

Repeat the sequence of lines between the `.rept` directive and the next `.endr` directive count times.

For example, assembling

            .rept   3
            .long   0
            .endr

is equivalent to assembling

            .long   0
            .long   0
            .long   0

## `.sbttl "subheading"`

Use subheading as the title (third line, immediately after the title line) when generating assembly listings.

This directive affects subsequent pages, as well as the current page if it appears within ten lines of the top of a page.

## `.scl class`

Set the storage-class value for a symbol. This directive may only be used inside a `.def`/`.endef` pair. Storage class may flag whether a symbol is static or external, or it may record further symbolic debugging information.

The ``.scl'` directive is primarily associated with COFF output; when configured to generate `b.out` output format, `as` accepts this directive but ignores it.

## `.section name`

Use the `.section` directive to assemble the following code into a section named name.

This directive is only supported for targets that actually support arbitrarily named sections; on `a.out` targets, for example, it is not accepted, even with a standard `a.out` section name.

For COFF targets, the `.section` directive is used in one of the following ways:

    .section name[, "flags"]
    .section name[, subsegment]

If the optional argument is quoted, it is taken as flags to use for the section. Each flag is a single character. The following flags are recognized:

`b`
  bss section (uninitialized data)
`n`
  section is not loaded
`w`
  writable section
`d`
  data section
`r`
  read-only section
`x`
  executable section

If no flags are specified, the default flags depend upon the section name. If the section name is not recognized, the default will be for the section to be loaded and writable.

If the optional argument to the `.section` directive is not quoted, it is taken as a subsegment number (see section Sub-Sections).

For ELF targets, the `.section` directive is used like this:

    .section name[, "flags"[, @type]]

The optional flags argument is a quoted string which may contain any combintion of the following characters:

`a`
  section is allocatable
`w`
  section is writable
`x`
  section is executable

The optional type argument may contain one of the following constants:

`@progbits`
  section contains data
`@nobits`
  section does not contain data (i.e., section only occupies space)

If no flags are specified, the default flags depend upon the section name. If the section name is not recognized, the default will be for the section to have none of the above flags: it will not be allocated in memory, nor writable, nor executable. The section will contain data.

For ELF targets, the assembler supports another type of `.section` directive for compatibility with the Solaris assembler:

    .section "name"[, flags...]

Note that the section name is quoted. There may be a sequence of comma separated flags:

`#alloc`
  section is allocatable
`#write`
  section is writable
`#execinstr`
  section is executable

## `.set symbol, expression`

Set the value of symbol to expression. This changes symbol's value and type to conform to expression. If symbol was flagged as external, it remains flagged (see section Symbol Attributes).

You may `.set` a symbol many times in the same assembly.

If you `.set` a global symbol, the value stored in the object file is the last value stored into it.

The syntax for `set` on the HPPA is ``symbol .set expression'`.

## `.short expressions`

`.short` is normally the same as ``.word'`. See section `.word expressions`.

In some configurations, however, `.short` and `.word` generate numbers of different lengths; see section Machine Dependent Features.

## `.single flonums`

This directive assembles zero or more flonums, separated by commas. It has the same effect as `.float`. The exact kind of floating point numbers emitted depends on how `as` is configured. See section Machine Dependent Features.

## `.size`

This directive is generated by compilers to include auxiliary debugging information in the symbol table. It is only permitted inside `.def`/`.endef` pairs.

``.size'` is only meaningful when generating COFF format output; when `as` is generating `b.out`, it accepts this directive but ignores it.

## `.skip size , fill`

This directive emits size bytes, each of value fill. Both size and fill are absolute expressions. If the comma and fill are omitted, fill is assumed to be zero. This is the same as ``.space'`.

## `.space size , fill`

This directive emits size bytes, each of value fill. Both size and fill are absolute expressions. If the comma and fill are omitted, fill is assumed to be zero. This is the same as ``.skip'`.

> Warning: `.space` has a completely different meaning for HPPA targets; use `.block` as a substitute. See HP9000 Series 800 Assembly Language Reference Manual (HP 92432-90001) for the meaning of the `.space` directive. See section HPPA Assembler Directives, for a summary.

On the AMD 29K, this directive is ignored; it is accepted for compatibility with other AMD 29K assemblers.

> Warning: In most versions of the GNU assembler, the directive `.space` has the effect of `.block` See section Machine Dependent Features.

## `.stabd, .stabn, .stabs`

There are three directives that begin ``.stab'`. All emit symbols (see section Symbols), for use by symbolic debuggers. The symbols are not entered in the `as` hash table: they cannot be referenced elsewhere in the source file. Up to five fields are required:

string
  This is the symbol's name. It may contain any character except ``\000'`, so is more general than ordinary symbol names. Some debuggers used to code arbitrarily complex structures into symbol names using this field.
type
  An absolute expression. The symbol's type is set to the low 8 bits of this expression. Any bit pattern is permitted, but `ld` and debuggers choke on silly bit patterns.
other
  An absolute expression. The symbol's "other" attribute is set to the low 8 bits of this expression.
desc
  An absolute expression. The symbol's descriptor is set to the low 16 bits of this expression.
value
  An absolute expression which becomes the symbol's value.

If a warning is detected while reading a `.stabd`, `.stabn`, or `.stabs` statement, the symbol has probably already been created; you get a half-formed symbol in your object file. This is compatible with earlier assemblers!

`.stabd type , other , desc`
  The "name" of the symbol generated is not even an empty string. It is a null pointer, for compatibility. Older assemblers used a null pointer so they didn't waste space in object files with empty strings. The symbol's value is set to the location counter, relocatably. When your program is linked, the value of this symbol is the address of the location counter when the `.stabd` was assembled.
`.stabn type , other , desc , value`
  The name of the symbol is set to the empty string `""`.
`.stabs string , type , other , desc , value`
  All five fields are specified.

## `.string` "str"

Copy the characters in str to the object file. You may specify more than one string to copy, separated by commas. Unless otherwise specified for a particular machine, the assembler marks the end of each string with a 0 byte. You can use any of the escape sequences described in section Strings.

## `.symver`

Use the `.symver` directive to bind symbols to specific version nodes within a source file. This is only supported on ELF platforms, and is typically used when assembling files to be linked into a shared library. There are cases where it may make sense to use this in objects to be bound into an application itself so as to override a versioned symbol from a shared library.

For ELF targets, the `.symver` directive is used like this:

    .symver name, name2@nodename

In this case, the symbol name must exist and be defined within the file being assembled. The `.versym` directive effectively creates a symbol alias with the name name2@nodename, and in fact the main reason that we just don't try and create a regular alias is that the @ character isn't permitted in symbol names. The name2 part of the name is the actual name of the symbol by which it will be externally referenced. The name name itself is merely a name of convenience that is used so that it is possible to have definitions for multiple versions of a function within a single source file, and so that the compiler can unambiguously know which version of a function is being mentioned. The nodename portion of the alias should be the name of a node specified in the version script supplied to the linker when building a shared library. If you are attempting to override a versioned symbol from a shared library, then nodename should correspond to the nodename of the symbol you are trying to override.

## `.tag structname`

This directive is generated by compilers to include auxiliary debugging information in the symbol table. It is only permitted inside `.def`/`.endef` pairs. Tags are used to link structure definitions in the symbol table with instances of those structures.

``.tag'` is only used when generating COFF format output; when `as` is generating `b.out`, it accepts this directive but ignores it.

## `.text subsection`

Tells `as` to assemble the following statements onto the end of the text subsection numbered subsection, which is an absolute expression. If subsection is omitted, subsection number zero is used.

## `.title "heading"`

Use heading as the title (second line, immediately after the source file name and pagenumber) when generating assembly listings.

This directive affects subsequent pages, as well as the current page if it appears within ten lines of the top of a page.

## `.type int`

This directive, permitted only within `.def`/`.endef` pairs, records the integer int as the type attribute of a symbol table entry.

``.type'` is associated only with COFF format output; when `as` is configured for `b.out` output, it accepts this directive but ignores it.

## `.val addr`

This directive, permitted only within `.def`/`.endef` pairs, records the address addr as the value attribute of a symbol table entry.

``.val'` is used only for COFF output; when `as` is configured for `b.out`, it accepts this directive but ignores it.

## `.word expressions`

This directive expects zero or more expressions, of any section, separated by commas.

The size of the number emitted, and its byte order, depend on what target computer the assembly is for.

> Warning: Special Treatment to support Compilers

Machines with a 32-bit address space, but that do less than 32-bit addressing, require the following special treatment. If the machine of interest to you does 32-bit addressing (or doesn't require it; see section Machine Dependent Features), you can ignore this issue.

In order to assemble compiler output into something that works, `as` occasionlly does strange things to ``.word'` directives. Directives of the form ``.word sym1-sym2'` are often emitted by compilers as part of jump tables. Therefore, when `as` assembles a directive of the form ``.word sym1-sym2'`, and the difference between `sym1` and `sym2` does not fit in 16 bits, `as` creates a secondary jump table, immediately before the next label. This secondary jump table is preceded by a short-jump to the first byte after the secondary table. This short-jump prevents the flow of control from accidentally falling into the new table. Inside the table is a long-jump to `sym2`. The original ``.word'` contains `sym1` minus the address of the long-jump to `sym2`.

If there were several occurrences of ``.word sym1-sym2'` before the secondary jump table, all of them are adjusted. If there was a ``.word sym3-sym4'`, that also did not fit in sixteen bits, a long-jump to `sym4` is included in the secondary jump table, and the `.word` directives are adjusted to contain `sym3` minus the address of the long-jump to `sym4`; and so on, for as many entries in the original jump table as necessary.

## Deprecated Directives

One day these directives won't work. They are included for compatibility with older assemblers.

`.abort`
`.app-file`
`.line`

Go to the first, previous, next, last section, table of contents.