This is doc/gccint.info, produced by makeinfo version 4.2 from
doc/gccint.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gccint: (gccint).            Internals of the GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the internals of the GNU compilers.

   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

   Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001, 2002 Free Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.


File: gccint.info,  Node: Expressions,  Next: Tagging Insns,  Prev: Defining Attributes,  Up: Insn Attributes

Attribute Expressions
---------------------

   RTL expressions used to define attributes use the codes described
above plus a few specific to attribute definitions, to be discussed
below.  Attribute value expressions must have one of the following
forms:

`(const_int I)'
     The integer I specifies the value of a numeric attribute.  I must
     be non-negative.

     The value of a numeric attribute can be specified either with a
     `const_int', or as an integer represented as a string in
     `const_string', `eq_attr' (see below), `attr', `symbol_ref',
     simple arithmetic expressions, and `set_attr' overrides on
     specific instructions (*note Tagging Insns::).

`(const_string VALUE)'
     The string VALUE specifies a constant attribute value.  If VALUE
     is specified as `"*"', it means that the default value of the
     attribute is to be used for the insn containing this expression.
     `"*"' obviously cannot be used in the DEFAULT expression of a
     `define_attr'.

     If the attribute whose value is being specified is numeric, VALUE
     must be a string containing a non-negative integer (normally
     `const_int' would be used in this case).  Otherwise, it must
     contain one of the valid values for the attribute.

`(if_then_else TEST TRUE-VALUE FALSE-VALUE)'
     TEST specifies an attribute test, whose format is defined below.
     The value of this expression is TRUE-VALUE if TEST is true,
     otherwise it is FALSE-VALUE.

`(cond [TEST1 VALUE1 ...] DEFAULT)'
     The first operand of this expression is a vector containing an even
     number of expressions and consisting of pairs of TEST and VALUE
     expressions.  The value of the `cond' expression is that of the
     VALUE corresponding to the first true TEST expression.  If none of
     the TEST expressions are true, the value of the `cond' expression
     is that of the DEFAULT expression.

   TEST expressions can have one of the following forms:

`(const_int I)'
     This test is true if I is nonzero and false otherwise.

`(not TEST)'
`(ior TEST1 TEST2)'
`(and TEST1 TEST2)'
     These tests are true if the indicated logical function is true.

`(match_operand:M N PRED CONSTRAINTS)'
     This test is true if operand N of the insn whose attribute value
     is being determined has mode M (this part of the test is ignored
     if M is `VOIDmode') and the function specified by the string PRED
     returns a nonzero value when passed operand N and mode M (this
     part of the test is ignored if PRED is the null string).

     The CONSTRAINTS operand is ignored and should be the null string.

`(le ARITH1 ARITH2)'
`(leu ARITH1 ARITH2)'
`(lt ARITH1 ARITH2)'
`(ltu ARITH1 ARITH2)'
`(gt ARITH1 ARITH2)'
`(gtu ARITH1 ARITH2)'
`(ge ARITH1 ARITH2)'
`(geu ARITH1 ARITH2)'
`(ne ARITH1 ARITH2)'
`(eq ARITH1 ARITH2)'
     These tests are true if the indicated comparison of the two
     arithmetic expressions is true.  Arithmetic expressions are formed
     with `plus', `minus', `mult', `div', `mod', `abs', `neg', `and',
     `ior', `xor', `not', `ashift', `lshiftrt', and `ashiftrt'
     expressions.

     `const_int' and `symbol_ref' are always valid terms (*note Insn
     Lengths::,for additional forms).  `symbol_ref' is a string
     denoting a C expression that yields an `int' when evaluated by the
     `get_attr_...' routine.  It should normally be a global variable.

`(eq_attr NAME VALUE)'
     NAME is a string specifying the name of an attribute.

     VALUE is a string that is either a valid value for attribute NAME,
     a comma-separated list of values, or `!' followed by a value or
     list.  If VALUE does not begin with a `!', this test is true if
     the value of the NAME attribute of the current insn is in the list
     specified by VALUE.  If VALUE begins with a `!', this test is true
     if the attribute's value is _not_ in the specified list.

     For example,

          (eq_attr "type" "load,store")

     is equivalent to

          (ior (eq_attr "type" "load") (eq_attr "type" "store"))

     If NAME specifies an attribute of `alternative', it refers to the
     value of the compiler variable `which_alternative' (*note Output
     Statement::) and the values must be small integers.  For example,

          (eq_attr "alternative" "2,3")

     is equivalent to

          (ior (eq (symbol_ref "which_alternative") (const_int 2))
               (eq (symbol_ref "which_alternative") (const_int 3)))

     Note that, for most attributes, an `eq_attr' test is simplified in
     cases where the value of the attribute being tested is known for
     all insns matching a particular pattern.  This is by far the most
     common case.

`(attr_flag NAME)'
     The value of an `attr_flag' expression is true if the flag
     specified by NAME is true for the `insn' currently being scheduled.

     NAME is a string specifying one of a fixed set of flags to test.
     Test the flags `forward' and `backward' to determine the direction
     of a conditional branch.  Test the flags `very_likely', `likely',
     `very_unlikely', and `unlikely' to determine if a conditional
     branch is expected to be taken.

     If the `very_likely' flag is true, then the `likely' flag is also
     true.  Likewise for the `very_unlikely' and `unlikely' flags.

     This example describes a conditional branch delay slot which can
     be nullified for forward branches that are taken (annul-true) or
     for backward branches which are not taken (annul-false).

          (define_delay (eq_attr "type" "cbranch")
            [(eq_attr "in_branch_delay" "true")
             (and (eq_attr "in_branch_delay" "true")
                  (attr_flag "forward"))
             (and (eq_attr "in_branch_delay" "true")
                  (attr_flag "backward"))])

     The `forward' and `backward' flags are false if the current `insn'
     being scheduled is not a conditional branch.

     The `very_likely' and `likely' flags are true if the `insn' being
     scheduled is not a conditional branch.  The `very_unlikely' and
     `unlikely' flags are false if the `insn' being scheduled is not a
     conditional branch.

     `attr_flag' is only used during delay slot scheduling and has no
     meaning to other passes of the compiler.

`(attr NAME)'
     The value of another attribute is returned.  This is most useful
     for numeric attributes, as `eq_attr' and `attr_flag' produce more
     efficient code for non-numeric attributes.


File: gccint.info,  Node: Tagging Insns,  Next: Attr Example,  Prev: Expressions,  Up: Insn Attributes

Assigning Attribute Values to Insns
-----------------------------------

   The value assigned to an attribute of an insn is primarily
determined by which pattern is matched by that insn (or which
`define_peephole' generated it).  Every `define_insn' and
`define_peephole' can have an optional last argument to specify the
values of attributes for matching insns.  The value of any attribute
not specified in a particular insn is set to the default value for that
attribute, as specified in its `define_attr'.  Extensive use of default
values for attributes permits the specification of the values for only
one or two attributes in the definition of most insn patterns, as seen
in the example in the next section.

   The optional last argument of `define_insn' and `define_peephole' is
a vector of expressions, each of which defines the value for a single
attribute.  The most general way of assigning an attribute's value is
to use a `set' expression whose first operand is an `attr' expression
giving the name of the attribute being set.  The second operand of the
`set' is an attribute expression (*note Expressions::) giving the value
of the attribute.

   When the attribute value depends on the `alternative' attribute
(i.e., which is the applicable alternative in the constraint of the
insn), the `set_attr_alternative' expression can be used.  It allows
the specification of a vector of attribute expressions, one for each
alternative.

   When the generality of arbitrary attribute expressions is not
required, the simpler `set_attr' expression can be used, which allows
specifying a string giving either a single attribute value or a list of
attribute values, one for each alternative.

   The form of each of the above specifications is shown below.  In
each case, NAME is a string specifying the attribute to be set.

`(set_attr NAME VALUE-STRING)'
     VALUE-STRING is either a string giving the desired attribute value,
     or a string containing a comma-separated list giving the values for
     succeeding alternatives.  The number of elements must match the
     number of alternatives in the constraint of the insn pattern.

     Note that it may be useful to specify `*' for some alternative, in
     which case the attribute will assume its default value for insns
     matching that alternative.

`(set_attr_alternative NAME [VALUE1 VALUE2 ...])'
     Depending on the alternative of the insn, the value will be one of
     the specified values.  This is a shorthand for using a `cond' with
     tests on the `alternative' attribute.

`(set (attr NAME) VALUE)'
     The first operand of this `set' must be the special RTL expression
     `attr', whose sole operand is a string giving the name of the
     attribute being set.  VALUE is the value of the attribute.

   The following shows three different ways of representing the same
attribute value specification:

     (set_attr "type" "load,store,arith")
     
     (set_attr_alternative "type"
                           [(const_string "load") (const_string "store")
                            (const_string "arith")])
     
     (set (attr "type")
          (cond [(eq_attr "alternative" "1") (const_string "load")
                 (eq_attr "alternative" "2") (const_string "store")]
                (const_string "arith")))

   The `define_asm_attributes' expression provides a mechanism to
specify the attributes assigned to insns produced from an `asm'
statement.  It has the form:

     (define_asm_attributes [ATTR-SETS])

where ATTR-SETS is specified the same as for both the `define_insn' and
the `define_peephole' expressions.

   These values will typically be the "worst case" attribute values.
For example, they might indicate that the condition code will be
clobbered.

   A specification for a `length' attribute is handled specially.  The
way to compute the length of an `asm' insn is to multiply the length
specified in the expression `define_asm_attributes' by the number of
machine instructions specified in the `asm' statement, determined by
counting the number of semicolons and newlines in the string.
Therefore, the value of the `length' attribute specified in a
`define_asm_attributes' should be the maximum possible length of a
single machine instruction.


File: gccint.info,  Node: Attr Example,  Next: Insn Lengths,  Prev: Tagging Insns,  Up: Insn Attributes

Example of Attribute Specifications
-----------------------------------

   The judicious use of defaulting is important in the efficient use of
insn attributes.  Typically, insns are divided into "types" and an
attribute, customarily called `type', is used to represent this value.
This attribute is normally used only to define the default value for
other attributes.  An example will clarify this usage.

   Assume we have a RISC machine with a condition code and in which only
full-word operations are performed in registers.  Let us assume that we
can divide all insns into loads, stores, (integer) arithmetic
operations, floating point operations, and branches.

   Here we will concern ourselves with determining the effect of an
insn on the condition code and will limit ourselves to the following
possible effects:  The condition code can be set unpredictably
(clobbered), not be changed, be set to agree with the results of the
operation, or only changed if the item previously set into the
condition code has been modified.

   Here is part of a sample `md' file for such a machine:

     (define_attr "type" "load,store,arith,fp,branch" (const_string "arith"))
     
     (define_attr "cc" "clobber,unchanged,set,change0"
                  (cond [(eq_attr "type" "load")
                             (const_string "change0")
                         (eq_attr "type" "store,branch")
                             (const_string "unchanged")
                         (eq_attr "type" "arith")
                             (if_then_else (match_operand:SI 0 "" "")
                                           (const_string "set")
                                           (const_string "clobber"))]
                        (const_string "clobber")))
     
     (define_insn ""
       [(set (match_operand:SI 0 "general_operand" "=r,r,m")
             (match_operand:SI 1 "general_operand" "r,m,r"))]
       ""
       "@
        move %0,%1
        load %0,%1
        store %0,%1"
       [(set_attr "type" "arith,load,store")])

   Note that we assume in the above example that arithmetic operations
performed on quantities smaller than a machine word clobber the
condition code since they will set the condition code to a value
corresponding to the full-word result.


File: gccint.info,  Node: Insn Lengths,  Next: Constant Attributes,  Prev: Attr Example,  Up: Insn Attributes

Computing the Length of an Insn
-------------------------------

   For many machines, multiple types of branch instructions are
provided, each for different length branch displacements.  In most
cases, the assembler will choose the correct instruction to use.
However, when the assembler cannot do so, GCC can when a special
attribute, the `length' attribute, is defined.  This attribute must be
defined to have numeric values by specifying a null string in its
`define_attr'.

   In the case of the `length' attribute, two additional forms of
arithmetic terms are allowed in test expressions:

`(match_dup N)'
     This refers to the address of operand N of the current insn, which
     must be a `label_ref'.

`(pc)'
     This refers to the address of the _current_ insn.  It might have
     been more consistent with other usage to make this the address of
     the _next_ insn but this would be confusing because the length of
     the current insn is to be computed.

   For normal insns, the length will be determined by value of the
`length' attribute.  In the case of `addr_vec' and `addr_diff_vec' insn
patterns, the length is computed as the number of vectors multiplied by
the size of each vector.

   Lengths are measured in addressable storage units (bytes).

   The following macros can be used to refine the length computation:

`FIRST_INSN_ADDRESS'
     When the `length' insn attribute is used, this macro specifies the
     value to be assigned to the address of the first insn in a
     function.  If not specified, 0 is used.

`ADJUST_INSN_LENGTH (INSN, LENGTH)'
     If defined, modifies the length assigned to instruction INSN as a
     function of the context in which it is used.  LENGTH is an lvalue
     that contains the initially computed length of the insn and should
     be updated with the correct length of the insn.

     This macro will normally not be required.  A case in which it is
     required is the ROMP.  On this machine, the size of an `addr_vec'
     insn must be increased by two to compensate for the fact that
     alignment may be required.

   The routine that returns `get_attr_length' (the value of the
`length' attribute) can be used by the output routine to determine the
form of the branch instruction to be written, as the example below
illustrates.

   As an example of the specification of variable-length branches,
consider the IBM 360.  If we adopt the convention that a register will
be set to the starting address of a function, we can jump to labels
within 4k of the start using a four-byte instruction.  Otherwise, we
need a six-byte sequence to load the address from memory and then
branch to it.

   On such a machine, a pattern for a branch instruction might be
specified as follows:

     (define_insn "jump"
       [(set (pc)
             (label_ref (match_operand 0 "" "")))]
       ""
     {
        return (get_attr_length (insn) == 4
                ? "b %l0" : "l r15,=a(%l0); br r15");
     }
       [(set (attr "length")
             (if_then_else (lt (match_dup 0) (const_int 4096))
                           (const_int 4)
                           (const_int 6)))])


File: gccint.info,  Node: Constant Attributes,  Next: Delay Slots,  Prev: Insn Lengths,  Up: Insn Attributes

Constant Attributes
-------------------

   A special form of `define_attr', where the expression for the
default value is a `const' expression, indicates an attribute that is
constant for a given run of the compiler.  Constant attributes may be
used to specify which variety of processor is used.  For example,

     (define_attr "cpu" "m88100,m88110,m88000"
      (const
       (cond [(symbol_ref "TARGET_88100") (const_string "m88100")
              (symbol_ref "TARGET_88110") (const_string "m88110")]
             (const_string "m88000"))))
     
     (define_attr "memory" "fast,slow"
      (const
       (if_then_else (symbol_ref "TARGET_FAST_MEM")
                     (const_string "fast")
                     (const_string "slow"))))

   The routine generated for constant attributes has no parameters as it
does not depend on any particular insn.  RTL expressions used to define
the value of a constant attribute may use the `symbol_ref' form, but
may not use either the `match_operand' form or `eq_attr' forms
involving insn attributes.


File: gccint.info,  Node: Delay Slots,  Next: Function Units,  Prev: Constant Attributes,  Up: Insn Attributes

Delay Slot Scheduling
---------------------

   The insn attribute mechanism can be used to specify the requirements
for delay slots, if any, on a target machine.  An instruction is said to
require a "delay slot" if some instructions that are physically after
the instruction are executed as if they were located before it.
Classic examples are branch and call instructions, which often execute
the following instruction before the branch or call is performed.

   On some machines, conditional branch instructions can optionally
"annul" instructions in the delay slot.  This means that the
instruction will not be executed for certain branch outcomes.  Both
instructions that annul if the branch is true and instructions that
annul if the branch is false are supported.

   Delay slot scheduling differs from instruction scheduling in that
determining whether an instruction needs a delay slot is dependent only
on the type of instruction being generated, not on data flow between the
instructions.  See the next section for a discussion of data-dependent
instruction scheduling.

   The requirement of an insn needing one or more delay slots is
indicated via the `define_delay' expression.  It has the following form:

     (define_delay TEST
                   [DELAY-1 ANNUL-TRUE-1 ANNUL-FALSE-1
                    DELAY-2 ANNUL-TRUE-2 ANNUL-FALSE-2
                    ...])

   TEST is an attribute test that indicates whether this `define_delay'
applies to a particular insn.  If so, the number of required delay
slots is determined by the length of the vector specified as the second
argument.  An insn placed in delay slot N must satisfy attribute test
DELAY-N.  ANNUL-TRUE-N is an attribute test that specifies which insns
may be annulled if the branch is true.  Similarly, ANNUL-FALSE-N
specifies which insns in the delay slot may be annulled if the branch
is false.  If annulling is not supported for that delay slot, `(nil)'
should be coded.

   For example, in the common case where branch and call insns require
a single delay slot, which may contain any insn other than a branch or
call, the following would be placed in the `md' file:

     (define_delay (eq_attr "type" "branch,call")
                   [(eq_attr "type" "!branch,call") (nil) (nil)])

   Multiple `define_delay' expressions may be specified.  In this case,
each such expression specifies different delay slot requirements and
there must be no insn for which tests in two `define_delay' expressions
are both true.

   For example, if we have a machine that requires one delay slot for
branches but two for calls,  no delay slot can contain a branch or call
insn, and any valid insn in the delay slot for the branch can be
annulled if the branch is true, we might represent this as follows:

     (define_delay (eq_attr "type" "branch")
        [(eq_attr "type" "!branch,call")
         (eq_attr "type" "!branch,call")
         (nil)])
     
     (define_delay (eq_attr "type" "call")
                   [(eq_attr "type" "!branch,call") (nil) (nil)
                    (eq_attr "type" "!branch,call") (nil) (nil)])


File: gccint.info,  Node: Function Units,  Prev: Delay Slots,  Up: Insn Attributes

Specifying Function Units
-------------------------

   On most RISC machines, there are instructions whose results are not
available for a specific number of cycles.  Common cases are
instructions that load data from memory.  On many machines, a pipeline
stall will result if the data is referenced too soon after the load
instruction.

   In addition, many newer microprocessors have multiple function
units, usually one for integer and one for floating point, and often
will incur pipeline stalls when a result that is needed is not yet
ready.

   The descriptions in this section allow the specification of how much
time must elapse between the execution of an instruction and the time
when its result is used.  It also allows specification of when the
execution of an instruction will delay execution of similar instructions
due to function unit conflicts.

   For the purposes of the specifications in this section, a machine is
divided into "function units", each of which execute a specific class
of instructions in first-in-first-out order.  Function units that
accept one instruction each cycle and allow a result to be used in the
succeeding instruction (usually via forwarding) need not be specified.
Classic RISC microprocessors will normally have a single function unit,
which we can call `memory'.  The newer "superscalar" processors will
often have function units for floating point operations, usually at
least a floating point adder and multiplier.

   Each usage of a function units by a class of insns is specified with
a `define_function_unit' expression, which looks like this:

     (define_function_unit NAME MULTIPLICITY SIMULTANEITY
                           TEST READY-DELAY ISSUE-DELAY
                          [CONFLICT-LIST])

   NAME is a string giving the name of the function unit.

   MULTIPLICITY is an integer specifying the number of identical units
in the processor.  If more than one unit is specified, they will be
scheduled independently.  Only truly independent units should be
counted; a pipelined unit should be specified as a single unit.  (The
only common example of a machine that has multiple function units for a
single instruction class that are truly independent and not pipelined
are the two multiply and two increment units of the CDC 6600.)

   SIMULTANEITY specifies the maximum number of insns that can be
executing in each instance of the function unit simultaneously or zero
if the unit is pipelined and has no limit.

   All `define_function_unit' definitions referring to function unit
NAME must have the same name and values for MULTIPLICITY and
SIMULTANEITY.

   TEST is an attribute test that selects the insns we are describing
in this definition.  Note that an insn may use more than one function
unit and a function unit may be specified in more than one
`define_function_unit'.

   READY-DELAY is an integer that specifies the number of cycles after
which the result of the instruction can be used without introducing any
stalls.

   ISSUE-DELAY is an integer that specifies the number of cycles after
the instruction matching the TEST expression begins using this unit
until a subsequent instruction can begin.  A cost of N indicates an N-1
cycle delay.  A subsequent instruction may also be delayed if an
earlier instruction has a longer READY-DELAY value.  This blocking
effect is computed using the SIMULTANEITY, READY-DELAY, ISSUE-DELAY,
and CONFLICT-LIST terms.  For a normal non-pipelined function unit,
SIMULTANEITY is one, the unit is taken to block for the READY-DELAY
cycles of the executing insn, and smaller values of ISSUE-DELAY are
ignored.

   CONFLICT-LIST is an optional list giving detailed conflict costs for
this unit.  If specified, it is a list of condition test expressions to
be applied to insns chosen to execute in NAME following the particular
insn matching TEST that is already executing in NAME.  For each insn in
the list, ISSUE-DELAY specifies the conflict cost; for insns not in the
list, the cost is zero.  If not specified, CONFLICT-LIST defaults to
all instructions that use the function unit.

   Typical uses of this vector are where a floating point function unit
can pipeline either single- or double-precision operations, but not
both, or where a memory unit can pipeline loads, but not stores, etc.

   As an example, consider a classic RISC machine where the result of a
load instruction is not available for two cycles (a single "delay"
instruction is required) and where only one load instruction can be
executed simultaneously.  This would be specified as:

     (define_function_unit "memory" 1 1 (eq_attr "type" "load") 2 0)

   For the case of a floating point function unit that can pipeline
either single or double precision, but not both, the following could be
specified:

     (define_function_unit
        "fp" 1 0 (eq_attr "type" "sp_fp") 4 4 [(eq_attr "type" "dp_fp")])
     (define_function_unit
        "fp" 1 0 (eq_attr "type" "dp_fp") 4 4 [(eq_attr "type" "sp_fp")])

   *Note:* The scheduler attempts to avoid function unit conflicts and
uses all the specifications in the `define_function_unit' expression.
It has recently come to our attention that these specifications may not
allow modeling of some of the newer "superscalar" processors that have
insns using multiple pipelined units.  These insns will cause a
potential conflict for the second unit used during their execution and
there is no way of representing that conflict.  We welcome any examples
of how function unit conflicts work in such processors and suggestions
for their representation.


File: gccint.info,  Node: Conditional Execution,  Next: Constant Definitions,  Prev: Insn Attributes,  Up: Machine Desc

Conditional Execution
=====================

   A number of architectures provide for some form of conditional
execution, or predication.  The hallmark of this feature is the ability
to nullify most of the instructions in the instruction set.  When the
instruction set is large and not entirely symmetric, it can be quite
tedious to describe these forms directly in the `.md' file.  An
alternative is the `define_cond_exec' template.

     (define_cond_exec
       [PREDICATE-PATTERN]
       "CONDITION"
       "OUTPUT-TEMPLATE")

   PREDICATE-PATTERN is the condition that must be true for the insn to
be executed at runtime and should match a relational operator.  One can
use `match_operator' to match several relational operators at once.
Any `match_operand' operands must have no more than one alternative.

   CONDITION is a C expression that must be true for the generated
pattern to match.

   OUTPUT-TEMPLATE is a string similar to the `define_insn' output
template (*note Output Template::), except that the `*' and `@' special
cases do not apply.  This is only useful if the assembly text for the
predicate is a simple prefix to the main insn.  In order to handle the
general case, there is a global variable `current_insn_predicate' that
will contain the entire predicate if the current insn is predicated,
and will otherwise be `NULL'.

   When `define_cond_exec' is used, an implicit reference to the
`predicable' instruction attribute is made.  *Note Insn Attributes::.
This attribute must be boolean (i.e. have exactly two elements in its
LIST-OF-VALUES).  Further, it must not be used with complex
expressions.  That is, the default and all uses in the insns must be a
simple constant, not dependent on the alternative or anything else.

   For each `define_insn' for which the `predicable' attribute is true,
a new `define_insn' pattern will be generated that matches a predicated
version of the instruction.  For example,

     (define_insn "addsi"
       [(set (match_operand:SI 0 "register_operand" "r")
             (plus:SI (match_operand:SI 1 "register_operand" "r")
                      (match_operand:SI 2 "register_operand" "r")))]
       "TEST1"
       "add %2,%1,%0")
     
     (define_cond_exec
       [(ne (match_operand:CC 0 "register_operand" "c")
            (const_int 0))]
       "TEST2"
       "(%0)")

generates a new pattern

     (define_insn ""
       [(cond_exec
          (ne (match_operand:CC 3 "register_operand" "c") (const_int 0))
          (set (match_operand:SI 0 "register_operand" "r")
               (plus:SI (match_operand:SI 1 "register_operand" "r")
                        (match_operand:SI 2 "register_operand" "r"))))]
       "(TEST2) && (TEST1)"
       "(%3) add %2,%1,%0")


File: gccint.info,  Node: Constant Definitions,  Prev: Conditional Execution,  Up: Machine Desc

Constant Definitions
====================

   Using literal constants inside instruction patterns reduces
legibility and can be a maintenance problem.

   To overcome this problem, you may use the `define_constants'
expression.  It contains a vector of name-value pairs.  From that point
on, wherever any of the names appears in the MD file, it is as if the
corresponding value had been written instead.  You may use
`define_constants' multiple times; each appearance adds more constants
to the table.  It is an error to redefine a constant with a different
value.

   To come back to the a29k load multiple example, instead of

     (define_insn ""
       [(match_parallel 0 "load_multiple_operation"
          [(set (match_operand:SI 1 "gpc_reg_operand" "=r")
                (match_operand:SI 2 "memory_operand" "m"))
           (use (reg:SI 179))
           (clobber (reg:SI 179))])]
       ""
       "loadm 0,0,%1,%2")

   You could write:

     (define_constants [
         (R_BP 177)
         (R_FC 178)
         (R_CR 179)
         (R_Q  180)
     ])
     
     (define_insn ""
       [(match_parallel 0 "load_multiple_operation"
          [(set (match_operand:SI 1 "gpc_reg_operand" "=r")
                (match_operand:SI 2 "memory_operand" "m"))
           (use (reg:SI R_CR))
           (clobber (reg:SI R_CR))])]
       ""
       "loadm 0,0,%1,%2")

   The constants that are defined with a define_constant are also output
in the insn-codes.h header file as #defines.


File: gccint.info,  Node: Target Macros,  Next: Host Config,  Prev: Machine Desc,  Up: Top

Target Description Macros and Functions
***************************************

   In addition to the file `MACHINE.md', a machine description includes
a C header file conventionally given the name `MACHINE.h' and a C
source file named `MACHINE.c'.  The header file defines numerous macros
that convey the information about the target machine that does not fit
into the scheme of the `.md' file.  The file `tm.h' should be a link to
`MACHINE.h'.  The header file `config.h' includes `tm.h' and most
compiler source files include `config.h'.  The source file defines a
variable `targetm', which is a structure containing pointers to
functions and data relating to the target machine.  `MACHINE.c' should
also contain their definitions, if they are not defined elsewhere in
GCC, and other functions called through the macros defined in the `.h'
file.

* Menu:

* Target Structure::    The `targetm' variable.
* Driver::              Controlling how the driver runs the compilation passes.
* Run-time Target::     Defining `-m' options like `-m68000' and `-m68020'.
* Per-Function Data::   Defining data structures for per-function information.
* Storage Layout::      Defining sizes and alignments of data.
* Type Layout::         Defining sizes and properties of basic user data types.
* Escape Sequences::    Defining the value of target character escape sequences
* Registers::           Naming and describing the hardware registers.
* Register Classes::    Defining the classes of hardware registers.
* Stack and Calling::   Defining which way the stack grows and by how much.
* Varargs::		Defining the varargs macros.
* Trampolines::         Code set up at run time to enter a nested function.
* Library Calls::       Controlling how library routines are implicitly called.
* Addressing Modes::    Defining addressing modes valid for memory operands.
* Condition Code::      Defining how insns update the condition code.
* Costs::               Defining relative costs of different operations.
* Scheduling::          Adjusting the behavior of the instruction scheduler.
* Sections::            Dividing storage into text, data, and other sections.
* PIC::			Macros for position independent code.
* Assembler Format::    Defining how to write insns and pseudo-ops to output.
* Debugging Info::      Defining the format of debugging output.
* Cross-compilation::   Handling floating point for cross-compilers.
* Mode Switching::      Insertion of mode-switching instructions.
* Target Attributes::   Defining target-specific uses of `__attribute__'.
* Misc::                Everything else.


File: gccint.info,  Node: Target Structure,  Next: Driver,  Up: Target Macros

The Global `targetm' Variable
=============================

 - Variable: struct gcc_target targetm
     The target `.c' file must define the global `targetm' variable
     which contains pointers to functions and data relating to the
     target machine.  The variable is declared in `target.h';
     `target-def.h' defines the macro `TARGET_INITIALIZER' which is
     used to initialize the variable, and macros for the default
     initializers for elements of the structure.  The `.c' file should
     override those macros for which the default definition is
     inappropriate.  For example:
          #include "target.h"
          #include "target-def.h"
          
          /* Initialize the GCC target structure.  */
          
          #undef TARGET_COMP_TYPE_ATTRIBUTES
          #define TARGET_COMP_TYPE_ATTRIBUTES MACHINE_comp_type_attributes
          
          struct gcc_target targetm = TARGET_INITIALIZER;

   Where a macro should be defined in the `.c' file in this manner to
form part of the `targetm' structure, it is documented below as a
"Target Hook" with a prototype.  Many macros will change in future from
being defined in the `.h' file to being part of the `targetm' structure.

