                         ===========================
                         = ptc conversion profiler =
                         ===========================


Overview
--------

This program profiles converter performance from 8/16/32bit -> all available
output formats. All conversion is done from SYSTEM -> VIDEO memory. Speeds
for SYSTEM->SYSTEM are higher. If a converter is listed as (n/a) it means that
the video mode could not be set (so the conversion could not be profiled).

Check it out, and see for yourself how fast PTC conversion routines are - It
really is practical to work virtually in 32bit, 16bit or 8bit!



NOTE: the profile program takes several minutes to execute, and may take a
      long time on slower machines such as 486s. You've been warned :)
