DOS/32 Advanced DOS Extender - Technical Reference 10.0 - DOS/32 Advanced - Values returned by DPMI function 0A00h Value returned by ADPMI function 0A00h, Vendor-Specific DPMI API Extensions in BL register, is DOS/32 Advanced built-in DPMI configuration. The format of the returned configuration is described below: `bit 0: 0=test DPMI/VCPI, 1=VCPI/DPMI /1=default bit 1: 0=internal exception control off, 1=on /1=default bit 2: 0=VCPI smartpage alloc mode off, 1=on /1=default bit 3: 0=VCPI+XMS alloc scheme off, 1=on /1=default bit 4: 0=trap emulated IRQs off, 1=on /1=default bit 5: 0=extended memory blocks checking off, 1=on /1=default bit 6: reserved bit 7: 0=ignore DOS/4G API calls off, 1=on /0=default` Please note that some of these settings may be altered by the user at run-time. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved