DOS/32 Advanced DOS Extender - Programmer's Reference 3.50 - DOS function 0FF92h - DOS/32 Advanced Free High Memory Block
In: | AX = 0FF92h ESI = handle of previously allocated memory block
Out: | if successful: CF clear if failed: CF set
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. b) This function is equal to DPMI function 0502h except that it uses 32-bit register instead of 16:16-bit pair of registers. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved