DOS/32 Advanced DOS Extender - Programmer's Reference 2.17 - DPMI function 0200h - Get Real Mode Interrupt Vector Returns the contents of the current virtual machine's real mode interrupt vector for the specified interrupt.
In: | AX = 0200h BL = interrupt number
Out: | CF clear CX:DX = segment:offset of real mode interrupt handler
Notes: a) The value returned in CX is a real mode segment address, not a selector. Attempts to place this value into a segment register in protected mode may cause a General Protection (GP) fault exception. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved