DOS/32 Advanced DOS Extender - Programmer's Reference 2.19 - DPMI function 0202h - Get Processor Exception Handler Vector Returns the address of the current client's protected mode exception handler for the specified exception number.
In: | AX = 0202h BL = exception number (00-1Fh)
Out: | if successful: CF clear CX:EDX = selector:offset of exception handler if failed: CF set AX = error code 8021h - invalid value (BL not in range 00-1Fh)
Notes: a) The value returned in CX is a valid protected mode selector, not a real mode segment address. b) DOS/32 Advanced DPMI supports only first 16 exceptions. Calls to this function with value in BL greater than 0Fh, but less than 1Fh, will return CX:EDX = 0 (0000:00000000h). c) DOS/32 Advanced DPMI does not handle exception 0Ch (Stack Fault). d) DOS/32 Advanced DPMI will read exceptions 08-0Fh from an internal buffer, not from IDT, when PIC master is mapped on these interrupts (INTs 08-0Fh). Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved