DOS/32 Advanced DOS Extender - Programmer's Reference 3.47 - DOS function 0FF8Ah - DOS/32 Advanced Get ADPMI Configuration Info
In: | AX = 0FF8Ah
Out: | EAX = 49443332h ('ID32') (if the function is supported) EBX = DOS/32 Advanced version number CL = CPU type 03h = 80386 04h = 80486 05h = 80586 (Pentium) 06h = 80686 (Pentium Pro or Pentium II) 07h-0FFh = reserved CH = System software type: 00h = Clean 01h = XMS 02h = VCPI 03h = DPMI DL = ADPMI Kernel configuration bits ESI = pointer to DOS/32 Advanced ADPMI Configuration Header FS = selector that can be used to access ADPMI Configuration Header
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. Additional information about value returned in DL register and about DOS/32 Advanced DPMI Kernel configuration can be found in the document "DOS/32 Advanced Technical Reference". Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved