DOS/32 Advanced DOS Extender - Programmer's Reference 2.06 - DPMI function 0007h - Set Segment Base Address Sets the 32-bit linear base address field in the descriptor table for the specified segment.
In: | AX = 0007h BX = selector CX:DX = 32-bit linear base address of segment
Out: | if successful: CF clear if failed: CF set AX = error code 8022h - invalid selector 8025h - invalid linear address (changing the base would cause the descriptor to reference a linear address range outside that allowed for DPMI clients)
Notes: a) DOS/32 Advanced DPMI and DPMI 1.0 hosts will automatically reload any segment register which contains the selector specified in register BX. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved