DOS/32 Advanced DOS Extender - Programmer's Reference 3.02 - DOS function 1Ah - Set DTA Address
In: | AH = 1Ah DS:EDX = pointer to DTA buffer DTA
Out: | -
Notes: a) DOS/32 Advanced allocates an internal DTA buffer in conventional memory. Each extended DOS function that accesses DTA will copy data from your DTA (pointed by DS:EDX) to this buffer, call real mode DOS function, and copy the updated data from the buffer back to your DTA. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved