DOS/32 Advanced DOS Extender - Programmer's Reference 4.02 - VGA function 1Ch - Save/Restore VGA State
In: | AH = 1Ch AL = subfunction: 00h - get state buffer size Returns: EBX = number of 64-byte blocks needed 01h - save video states 02h - restore video states ECX = states to save/restore: bit 0 - VGA video hardware state bit 1 - VGA BIOS data state bit 2 - VGA DAC state ES:EBX = pointer to save/restore buffer
Out: | AL = 1Ch (if function supported by VGA BIOS)
Notes: a) many BIOSes corrupt the video registers when saving the state, so a program should restore the state immediately after saving it (the saved data is uncorrupted). b) For subfunctions 01h and 02h, the DOS Extender will internally call subfunction 00h to extract the information about size of data that is to be copied. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved