DOS/32 Advanced DOS Extender - Programmer's Reference 4.03 - VBE function 4F00h - Get SuperVGA Information
In: | AX = 4F00h ES:EDI = pointer to 512 byte buffer
Out: | AL = 4Fh (if function supported by VESA BIOS) AH = 00h (if function was successful) ES:EDI = pointer to 512 byte buffer filled with VESA BIOS information
Notes: a) The following fields in the structure pointed to by ES:EDI will be converted to protected mode linear pointers relative to 0: OemStringPtr at offset 06h VideoModePtr at offset 0Eh OemVendorNamePtr at offset 16h OemProductNamePtr at offset 1Ah OemProductRevPtr at offset 1Eh Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved