DOS/32 Advanced DOS Extender - Programmer's Reference 4.06 - VBE function 4F09h - Load/Unload Palette Data
In: | AX = 4F09h BL = subfunction: 00h - set palette data 01h - get palette data 02h - set 2nd palette data 03h - get 2nd palette data 80h - set palette data during VR ECX = number of palette registers to update EDX = first palette register to update ES:EDI = pointer to buffer that contains palette data
Out: | AL = 4Fh (if function supported by VESA BIOS) AH = 00h (if function was successful)
Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved