Overview Servers and Relays Addresses Macros Options How To.. Menus Index |  |  | # Choose Server Configuration You can choose to configure your server as either a DHCP server or as a BOOTP relay agent. The DHCP server manages the IP address space of networks connected to the server. The BOOTP relay agent can receive requests for configuration from a client in a network not directly connected to a DHCP server and forward the request to a DHCP server.