!==
!== BROWSING-Config.txt for Samba release 2.2.0-alpha3 24 Mar 2001
!==
Date:		July 5, 1998
Contributor:	John H Terpstra <jht@samba.org>

Subject:	Cross Subnet Browsing / Cross Workgroup Browsing
===============================================================================

OVERVIEW:
=========

This document should be read in conjunction with BROWSING.txt and may
be taken as the fast track guide to implementing browsing across subnets
and / or across workgroups (or domains). WINS is the best tool for resolution
of NetBIOS names to IP addesses. WINS is NOT involved in browse list handling
except by way of name to address mapping.


DISCUSSION:
===========

Firstly, all MS Windows networking is based on SMB (Server Message
Block) based messaging. SMB messaging is implemented using NetBIOS. Samba
implements NetBIOS by encapsulating it over TCP/IP. MS Windows products can
do likewise. NetBIOS based networking uses broadcast messaging to affect
browse list management. When running NetBIOS over TCP/IP this uses UDP
based messaging. UDP messages can be broadcast or unicast.

Normally, only unicast UDP messaging can be forwarded by routers. The
"remote announce" parameter to smb.conf helps to project browse announcements
to remote network segments via unicast UDP. Similarly, the "remote browse sync"
parameter of smb.conf implements browse list collation using unicast UDP.

Secondly, in those networks where Samba is the only SMB server technology
wherever possible nmbd should be configured on one (1) machine as the WINS
server. This makes it easy to manage the browsing environment. If each network
segment is configured with it's own Samba WINS server, then the only way to
get cross segment browsing to work is by using the "remote announce" and
the "remote browse sync" parameters to your smb.conf file.

If only one WINS server is used then the use of the "remote announce" and the
"remote browse sync" parameters should NOT be necessary.

Samba WINS does not support MS-WINS replication. This means that when setting up
Samba as a WINS server there must only be one nmbd configured as a WINS server
on the network. Some sites have used multiple Samba WINS servers for redundancy
(one server per subnet) and then used "remote browse sync" and "remote announce"
to affect browse list collation across all segments. Note that this means
clients will only resolve local names, and must be configured to use DNS to
resolve names on other subnets in order to resolve the IP addresses of the
servers they can see on other subnets. This setup is not recommended, but is
mentioned as a practical consideration (ie: an 'if all else fails' scenario).

Lastly, take note that browse lists are a collection of unreliable broadcast
messages that are repeated at intervals of not more than 15 minutes. This means
that it will take time to establish a browse list and it can take up to 45
minutes to stabilise, particularly across network segments.


A) Use of the "Remote Announce" parameter
------------------------------------------
The "remote announce" parameter of smb.conf can be used to forcibly ensure
that all the NetBIOS names on a network get announced to a remote network.
The syntax of the "remote announce" parameter is:

	remote announce = a.b.c.d [e.f.g.h] ...
_or_
	remote announce = a.b.c.d/WORKGROUP [e.f.g.h/WORKGROUP] ...

where:
	a.b.c.d:	is either the LMB (Local Master Browser) IP address
	e.f.g.h:	or the broadcst address of the remote network.
			ie: the LMB is at 192.168.1.10, or the address
			could be given as 192.168.1.255 where the netmask
			is assumed to be 24 bits (255.255.255.0).
			When the remote announcement is made to the broadcast
			address of the remote network every host will receive
			our announcements. This is noisy and therefore
			undesirable but may be necessary if we do NOT know
			the IP address of the remote LMB.

	WORKGROUP:	is optional and can be either our own workgroup
			or that of the remote network. If you use the
			workgroup name of the remote network then our
			NetBIOS machine names will end up looking like
			they belong to that workgroup, this may cause
			name resolution problems and should be avoided.


B) Use of the "Remote Browse Sync" parameter
--------------------------------------------

The "remote browse sync" parameter of smb.conf is used to announce to
another LMB that it must synchronise it's NetBIOS name list with our
Samba LMB. It works ONLY if the Samba server that has this option is
simultaneously the LMB on it's network segment.

The syntax of the "remote browse  sync" parameter is:

	remote browse sync = a.b.c.d

where:
	a.b.c.d:	is either the IP address of the remote LMB or else
			is the network broadcast address of the remote segment.


C) Use of WINS
--------------

Use of WINS (either Samba WINS _or_ MS Windows NT Server WINS) is highly
recommended. Every NetBIOS machine registers it's name together with a
name_type value for each of of several types of service it has available.
eg: It registers it's name directly as a unique (the type 0x03) name.
It also registers it's name if it is running the lanmanager compatible
server service (used to make shares and printers available to other users)
by registering the server (the type 0x20) name.

All NetBIOS names are up to 15 characters in length. The name_type variable
is added to the end of the name - thus creating a 16 character name. Any
name that is shorter than 15 characters is padded with spaces to the 15th
character. ie: All NetBIOS names are 16 characters long (including the
name_type information).

WINS can store these 16 character names as they get registered. A client
that wants to log onto the network can ask the WINS server for a list
of all names that have registered the NetLogon service name_type. This saves
broadcast traffic and greatly expedites logon processing. Since broadcast
name resolution can not be used across network segments this type of
information can only be provided via WINS _or_ via statically configured
"lmhosts" files that must reside on all clients in the absence of WINS.

WINS also serves the purpose of forcing browse list synchronisation by all
LMB's. LMB's must synchronise their browse list with the DMB (domain master
browser) and WINS helps the LMB to identify it's DMB. By definition this
will work only within a single workgroup. Note that the domain master browser
has NOTHING to do with what is referred to as an MS Windows NT Domain. The
later is a reference to a security environment while the DMB refers to the
master controller for browse list information only.

Use of WINS will work correctly only if EVERY client TCP/IP protocol stack
has been configured to use the WINS server/s. Any client that has not been
configured to use the WINS server will continue to use only broadcast based
name registration so that WINS may NEVER get to know about it. In any case,
machines that have not registered with a WINS server will fail name to address
lookup attempts by other clients and will therefore cause workstation access
errors.

To configure Samba as a WINS server just add "wins support = yes" to the
smb.conf file [globals] section.

To configure Samba to register with a WINS server just add
"wins server = a.b.c.d" to your smb.conf file [globals] section.

DO NOT EVER use both "wins support = yes" together with "wins server = a.b.c.d"
particularly not using it's own IP address.


D) Do NOT use more than one (1) protocol on MS Windows machines
---------------------------------------------------------------

A very common cause of browsing problems results from installing more than
one protocol on an MS Windows machine.

Every NetBIOS machine take part in a process of electing the LMB (and DMB)
every 15 minutes. A set of election criteria is used to determine the order
of precidence for winning this election process. A machine running Samba or
Windows NT will be biased so that the most suitable machine will predictably
win and thus retain it's role.

The election process is "fought out" so to speak over every NetBIOS network
interface. In the case of a Windows 9x machine that has both TCP/IP and IPX
installed and has NetBIOS enabled over both protocols the election will be
decided over both protocols. As often happens, if the Windows 9x machine is
the only one with both protocols then the LMB may be won on the NetBIOS
interface over the IPX protocol. Samba will then lose the LMB role as Windows
9x will insist it knows who the LMB is. Samba will then cease to function
as an LMB and thus browse list operation on all TCP/IP only machines will
fail.

The safest rule of all to follow it this - USE ONLY ONE PROTOCOL!


E) Name Resolution Order
========================

Resolution of NetBIOS names to IP addresses can take place using a number
of methods. The only ones that can provide NetBIOS name_type information
are:
	WINS:		the best tool!
	LMHOSTS:	is static and hard to maintain.
	Broadcast:	uses UDP and can not resolve names across
			remote segments.

Alternative means of name resolution includes:
	/etc/hosts:	is static, hard to maintain, and lacks name_type info.
	DNS:		is a good choice but lacks essential name_type info.

Many sites want to restrict DNS lookups and want to avoid broadcast name
resolution traffic. The "name resolve order" parameter is of great help here.
The syntax of the "name resolve order" parameter is:

	name resolve order = wins lmhosts bcast host
_or_
	name resolve order = wins lmhosts  	(eliminates bcast and host)

the default is:
	name  resolve order = host lmhost wins bcast

where:
	"host" refers the the native methods used by the Unix system
	to implement the gethostbyname() function call. This is normally
	controlled by:
		/etc/host.conf
		/etc/nsswitch.conf
		/etc/resolv.conf

===============================================================================
