DOS/32 Advanced DOS Extender - Programmer's Reference 3.07 - DOS function 2Fh - Get DTA buffer
In: | AH = 2Fh
Out: | ES:EBX = pointer to DTA buffer
Notes: a) This function returns the pointer that was previously set by DOS function 1Ah, or the pointer to the default buffer that was allocated by DOS/32 Advanced if DOS function 1Ah was never called. Copyright © DOS/32 Advanced Team 1996-2002 All Rights Reserved