OBSOLETE Patch-ID# 113573-04
Keywords: psvc_sema_rdwr picld segmentation fault v880 i2c queries
Synopsis: Obsoleted by: 113573-05 SunOS 5.9: libpsvc Patch
Date: Mar/03/2004


Install Requirements: Reboot after installation                      
                      
Solaris Release: 9

SunOS Release: 5.9

Unbundled Product: 

Unbundled Release: 

Xref: 

Topic: SunOS 5.9: libpsvc Patch

Relevant Architectures: sparc

BugId's fixed with this patch: 4487110 4640559 4660073 4661192 4718737 4796100 4801542

Changes incorporated in this version: 4801542

Patches accumulated and obsoleted by this patch: 113025-01

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/usr/platform/SUNW,Sun-Fire-280R/lib/libpsvcpolicy_psr.so.1
/usr/platform/SUNW,Sun-Fire-280R/lib/picl/plugins/libpsvcplugin.so.1
/usr/platform/sun4u/lib/libpsvcobj.so.1
/usr/platform/sun4u/lib/libpsvcpolicy.so.1

Problem Description:

4801542 picld needs hardening against "false positives" due to the nature of I2C bus
 
(from 113573-03)
 
4796100 psvcplugin segmentation fault during picld stop
 
(from 113573-02)
 
4660073 picld messages not seen upon boot in dual CPU systems
4661192 "picld" process spending too much of CPU time cumulatively, on V880
 
(from 113573-01)
 
4487110 failure to open semaphore /psvc_sema_rdwr on reboot
4718737 PICLD incorrectly detects a CPU module when a Zulu module is present in the slot
 
(from 113025-01)
 
4640559 Spurious "No FRU Information for CPU1_DIE_TEMPERATURE_SENSOR" message

Patch Installation Instructions:
--------------------------------
 
For Solaris 2.0-2.6 releases, refer to the Install.info file and/or
the README within the patch for instructions on using the generic
'installpatch' and 'backoutpatch' scripts provided with each patch.
 
For Solaris 7-9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
       example# patchadd /var/spool/patch/104945-02
 
The following example removes a patch from a standalone system:
 
       example# patchrm 104945-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
 
NOTE 1 : To get the complete fix for bug 4487110 please install the following
         patch:
 
         113574-02 (or newer)    PICL support for SUNW,Sun-Fire-880 (only
			       for Daktari platform)
 
         The application of this patch will require the user to also add
         patches for SunVTS for this code to work.
 
	 SunVTS Version        Patch ID                OS release
	 ---------------       --------                ----------
	 sunvts version 5.0    113500-01 or later      Solaris 9
 
NOTE 2 : 
 
	a) If installing this patch (113573-04 or newer) on a Sun-Fire-480R,
	   please also install 114864-01 (or newer).
 
	b) If installing this patch (113573-04 or newer) on a Sun-Fire-880,
	   please also install 113574-07 (or newer).

README -- Last modified date:  Tuesday, June 8, 2004

